# Class CIM_LogicalModule
extends CIM_LogicalDevice

LogicalModule is the logical device that corresponds to a component part (such as a card or blade) in a device. For example, a line card in a switch is an instance of LogicalModule, that is associated with the the switch itself. A logical module is not necessarily independently managed.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_LogicalModule

## Direct Known Subclasses

CIM_PassThroughModule

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | LogicalModule is the logical device that corresponds to a component part (such as a card or blade) in a device. For example, a line card in a switch is an instance of LogicalModule, that is associated with the the switch itself. A logical module is not necessarily independently managed.
UMLPackagePath | string | CIM::Device::Ports
Version | string | 2.22.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
LogicalModuleType | uint16 | 0
Description | string | Type identifies the type of LogicalModule this instance represents. A value of "Unknown" indicates that the LogicalModuleType is unknown. A value of "Other" indicates that the value is not one of the enumerated values. OtherLogicalModuleTypeDescription should contain additional information. A value of "Device Tray" indicates that the device is a device or media tray, for example in a modular system. A value of "Line Card" indicates that the module is a line card in a switch. A value of "Blade" indicates the module is a blade inserted into a switch. The ranges expressed by "DMTF Reserved" and "Vendor Reserved" are reserved for DMTF and Vendor extensibility, respectively.
ModelCorrespondence | string | CIM_LogicalModule.OtherLogicalModuleTypeDescription
ValueMap | string | 0, 1, 2, 3, 4, 5..32767, 32768..65535
Values | string | Unknown, Other, Device Tray, Line Card, Blade, DMTF Reserved, Vendor Reserved
ModuleNumber | uint16 |
Description | string | Logical modules are often named by the physical or logical slot that they occupy within the containing device. ModuleNumber is the number assigned to the module by its parent.
OtherLogicalModuleTypeDescription | string |
Description | string | OtherLogicalModuleTypeDescription provides additional information about the type of LogicalModule represented by this instance when the value of LogicalModuleType is 1 ("Other").
ModelCorrespondence | string | CIM_LogicalModule.LogicalModuleType

### Inherited Properties

Name | Data Type
--- | ---
AllocationState | string
Availability | uint16
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
DeviceID | string
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
ErrorCleared | boolean
ErrorDescription | string
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LastErrorCode | uint32
LocationIndicator | uint16
MaxQuiesceTime | uint64
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PowerManagementSupported | boolean
PowerOnHours | uint64
PrimaryStatus | uint16
RequestedState | uint16
Status | string
StatusInfo | uint16
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TotalPowerOnHours | uint64
TransitioningToState | uint16
AdditionalAvailability | uint16[]
AvailableRequestedStates | uint16[]
IdentifyingDescriptions | string[]
OperationalStatus | uint16[]
OtherIdentifyingInfo | string[]
PowerManagementCapabilities | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
EnableDevice | uint32
OnlineDevice | uint32
QuiesceDevice | uint32
RequestStateChange | uint32
Reset | uint32
RestoreProperties | uint32
SaveProperties | uint32
SetPowerState | uint32