# Class CIM_Priority8021QMarkerService
extends CIM_MarkerService

Priority8021QMarkerService marks the Priority field in an 802.1Q- compliant frame, with a specified value. Frames are marked in order to control the conditioning that they will subsequently receive. Following common practice, the value to be written into the field is represented as an unsigned 8-bit integer.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_ConditioningService
|
+--CIM_MarkerService
|
+--CIM_Priority8021QMarkerService

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Priority8021QMarkerService marks the Priority field in an 802.1Q- compliant frame, with a specified value. Frames are marked in order to control the conditioning that they will subsequently receive. Following common practice, the value to be written into the field is represented as an unsigned 8-bit integer.
UMLPackagePath | string | CIM::Network::QoS
Version | string | 2.7.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
PriorityValue | uint8 |
Description | string | This property is an unsigned 8-bit integer, representing a value to be used for marking the Priority field in the 802.1Q header. Since the Priority field consists of 3 bits, the values for this property are limited to the range 0..7. When the Priority field is marked, the remaining two bits in the octet are left unchanged.
MaxValue | sint64 | 7
MinValue | sint64 | 0

### Inherited Properties

Name | Data Type
--- | ---
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
ElementName | string
Enabled | boolean
EnabledDefault | uint16
EnabledState | uint16
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LoSID | string
LoSOrgID | string
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PrimaryOwnerContact | string
PrimaryOwnerName | string
PrimaryStatus | uint16
RequestedState | uint16
Started | boolean
StartMode | string
Status | string
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TransitioningToState | uint16
AvailableRequestedStates | uint16[]
OperationalStatus | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
ChangeAffectedElementsAssignedSequence | uint32
RequestStateChange | uint32
StartService | uint32
StopService | uint32