# Class CIM_Unimodem
extends CIM_POTSModem

Unimodem is a POTSModem that supports the Unimodem 1.0 Specification.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_Modem
|
+--CIM_CallBasedModem
|
+--CIM_POTSModem
|
+--CIM_Unimodem

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Unimodem is a POTSModem that supports the Unimodem 1.0 Specification.
UMLPackagePath | string | CIM::Device::Modems
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
CallSetupResultCode | uint16 |
Description | string | Current call setup result code.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11
Values | string | No Previous Call, No Dial Tone Detected, Reorder Signal Detected, Network Busy, Busy Signal Detected, No Recognized Signal Detected, Voice Detected, Text Telephone Detected, Data Answering Signal Detected, Data Calling Signal Detected, Fax Answering Signal Detected, Fax Calling Signal Detected, V.8bis Signal Detected
CallWaitingEventCount | uint8 |
Counter | boolean | true
Description | string | Number of Call waiting events detected for the last or current call.
CarrierRenegotiationEventCount | uint8 |
Counter | boolean | true
Description | string | Carrier Rate renegotiation event count for the last or current call.
CarrierRetrainsGranted | uint8 |
Counter | boolean | true
Description | string | The number of carrier retrains granted during the current or last call.
CarrierRetrainsRequested | uint8 |
Counter | boolean | true
Description | string | The number of carrier retrains requested during the current or last call.
DTEDCEInterfaceMode | uint16 |
Description | string | Current DTE-DCE interface mode of the Unimodem, such as asynchronous, V.80 transparent, or framed synchronous modes.
ValueMap | string | 0, 1, 2
Values | string | Async Data, V.80 Transparent Synchronous Mode, V.80 Framed Synchronous Mode
ErrorControlFrameSize | uint16 |
Description | string | Error Control frame size in bytes for the last or current call.
PUnit | string | byte
Units | string | Bytes
ErrorControlLinkNAKs | uint8 |
Counter | boolean | true
Description | string | Error control link NAKs received for the last or current call.
ErrorControlLinkTimeouts | uint8 |
Counter | boolean | true
Description | string | Error control link timeouts in transmission for the last or current call.
EstimatedNoiseLevel | uint32 |
Description | string | Estimated noise level for the last or current call in -dBm. Values are in the range of 0-100.
Gauge | boolean | true
PUnit | string | decibel(m) * -1
Units | string | -dBm
FinalReceiveCarrierDataRate | uint32 |
Description | string | Final receive carrier data rate of the current or last call, in bits per second.
PUnit | string | bit / second
Units | string | Bits per Second
FinalTransmitCarrierDataRate | uint32 |
Description | string | Final transmit carrier data rate of the current or last call, in bits per second.
PUnit | string | bit / second
Units | string | Bits per Second
InitialReceiveCarrierDataRate | uint32 |
Description | string | Initial receive carrier data rate for the current or last call, in bits per second.
PUnit | string | bit / second
Units | string | Bits per Second
InitialTransmitCarrierDataRate | uint32 |
Description | string | Initial transmit carrier data rate for the current or last call, in bits per second.
PUnit | string | bit / second
Units | string | Bits per Second
MultiMediaMode | uint16 |
Description | string | Current multimedia mode of the Unimodem.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10
Values | string | Data Only, Fax Only, Voice Only, Voice View, ASVD V.61, ASVD V.34Q, DSVD Multi-Tech, DSVD 1.2, DSVD V.70, Video Telephony H.324, Other V.80 Call
NormalizedMeanSquaredError | uint32 |
Description | string | Normalized mean squared error for the last or current call.
ReceiveCarrierNegotiation | uint16 |
Description | string | The active receive modulation scheme.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23..65535
Values | string | V.17 (G3 Fax Call), V.21, V.22, V.22bis, V.23 Constant Carrier (1200/75), V.23 Switched Carrier (Half Duplex), V.26bis, V.26ter, V.27ter (G3 Fax Call), V.29 HD (G3 Fax Call), V.32, V.32bis, V.34, V.34 HD (G3 Fax Call), V.90 Issue 1 (Asymmetric), V.90 Issue 2 (Symmetric), Reserved (V.58), X2, K56FLEX, V.FC, V.32terbo, Bell 212A, Bell 103, Reserved for Mfgs
ReceiveCharsLost | uint64 |
Counter | boolean | true
Description | string | Number of receive characters lost for the last or current call. A DCE might limit this counter to 16 bits, but additional bits can be provided and are accounted for in this property.
ReceiveCharsSentToDTE | uint64 |
Counter | boolean | true
Description | string | Number of receive chars sent to the DTE for the last or current call. A continuous connection might exceed this value, given enough time. Typically these counters are implemented as 32-bit counters, but additional bits can be provided and are accounted for in this property. If these counters hit maximum value, the DCE manufacturer might roll over to 0.
ReceivedIFrameErrorCount | uint64 |
Counter | boolean | true
Description | string | Number of I-Frame errors detected for the last or current call, if error control protocol is running. A DCE might limit this counter to 16 bits, but additional bits can be provided and are accounted for in this property.
ReceiveFlowControl | uint16 |
Description | string | The flow control mechanism used in receiving data.
ValueMap | string | 0, 1, 2, 3
Values | string | Unknown, Off, DC1/DC3, V.24 ckt 106/133
ReceiveIFrameCount | uint64 |
Counter | boolean | true
Description | string | Number of I-Frames received for the last or current call. A continuous connection might exceed this value, given enough time. Typically these counters are implemented as 32-bit counters, but additional bits can be provided and are accounted for in this property. If these counters hit maximum value, the DCE manufacturer might roll over to 0.
TemporaryCarrierLossEventCount | uint8 |
Counter | boolean | true
Description | string | Temporary carrier loss event count for the last or current call.
TerminationCause | uint16 |
Description | string | Cause of last call termination.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23, 24, 25, 26, 27, 28, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 43, 44, 45, 46, 47, 48, 49, 50
Values | string | Cause Unidentified, No Previous Call, Call Is Still in Progress, Call Waiting Signal Detected, Delayed, NMS Initiated Dial Call, NMS Initiated Leased Line Restoral, NMS Initiated Redial, NMS Initiated Dial Disconnect, Power Loss, Equipment Failure, Front Panel Disconnect Requested, Front Panel Leased Line Restoral, Automatic Leased Line Restoral, Inactivity Timer Expired, cct116 Restoral Request, cct108 Is Off Inhibits Dial, cct108 Turned Off, No Number Provided, Blacklisted Number, Call Attempts Limit Exceeded, Extension Phone Off Hook, Call Setup Fail Timer Expired, Incoming Call Detected, Loop Current Interrupted, No Dial Tone, Voice Detected, Reorder Tone, Sit Tone, Engaged Tone, Long Space Disconnect, Carrier Lost, Training Failed, No Modulation in Common, Retrain Failed, Retrain Attempt Count Exceeded, GSTN Cleardown Received, Fax Detected, In Test Mode, Intrusive Self Test Initiated, Any Key Abort, DTE Hangup Command, DTE Reset Command, Frame Reject, No Error Control Established, Protocol Violation, n400 Exceeded, Negotiation Failed, Disconnect Frame Received, Sabme Frame Received, Loss Of Synchronization
TransmitCarrierNegotiation | uint16 |
Description | string | The active transmit modulation scheme.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23..65535
Values | string | V.17 (G3 Fax Call), V.21, V.22, V.22bis, V.23 Constant Carrier (1200/75), V.23 Switched Carrier (Half Duplex), V.26bis, V.26ter, V.27ter (G3 Fax Call), V.29 HD (G3 Fax Call), V.32, V.32bis, V.34, V.34 HD (G3 Fax Call), V.90 Issue 1 (Asymmetric), V.90 Issue 2 (Symmetric), Reserved (V.58), X2, K56FLEX, V.FC, V.32terbo, Bell 212A, Bell 103, Reserved for Mfgs
TransmitCharsLost | uint64 |
Counter | boolean | true
Description | string | Number of transmit characters lost for the last or current call. A DCE might limit this counter to 16 bits, but additional bits can be provided and are accounted for in this property.
TransmitCharsSentFromDTE | uint64 |
Counter | boolean | true
Description | string | Number of transmit chars sent from the DTE for the last or current call. A continuous connection might exceed this value, given enough time. Typically these counters are implemented as 32-bit counters, but additional bits can be provided and are accounted for in this property. If these counters hit maximum value, the DCE manufacturer might roll over to 0.
TransmitFlowControl | uint16 |
Description | string | The flow control mechanism used in transmitting data.
ValueMap | string | 0, 1, 2, 3
Values | string | Unknown, Off, DC1/DC3, V.24 ckt 106/133
TransmitIFrameCount | uint64 |
Counter | boolean | true
Description | string | Number of I-Frames transmitted for the last or current call. A continuous connection might exceed this value, given enough time. Typically these counters are implemented as 32- bit counters, but additional bits can be provided and are accounted for in this property. If these counters hit maximum value, the DCE manufacturer might roll over to 0.
TransmitIFrameErrorCount | uint64 |
Counter | boolean | true
Description | string | Number of I-Frame errors detected for the last or current call, if error control protocol is running. A DCE might limit this counter to 16 bits, but additional bits can be provided and are accounted for in this property.
UnimodemRevision | string |
Description | string | Diagnostic Command Specification, Unimodem revision number.

### Inherited Properties

Name | Data Type
--- | ---
AllocationState | string
AnswerMode | uint16
Availability | uint16
BlockErrors | uint32
BlocksReceived | uint32
BlocksResent | uint32
BlocksSent | uint32
CallLength | datetime
CallSpeed | uint32
CallStatus | uint16
Caption | string
CharsLost | uint32
CharsReceived | uint32
CharsSent | uint32
CommunicationStatus | uint16
CompressionInfo | uint16
CountrySelected | string
CreationClassName | string
Description | string
DetailedStatus | uint16
DeviceID | string
DialType | uint16
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
Equalization | uint16
ErrorCleared | boolean
ErrorControlInfo | uint16
ErrorDescription | string
FallbackEnabled | boolean
Generation | uint64
HealthState | uint16
InactivityTimeout | uint32
InstallDate | datetime
InstanceID | string
LastErrorCode | uint32
LocationIndicator | uint16
MaxBaudRateToPhone | uint32
MaxBaudRateToSerialPort | uint32
MaxNumberOfPasswords | uint16
MaxQuiesceTime | uint64
ModulationScheme | uint16
Name | string
NumberDialed | string
OperatingStatus | uint16
OtherCompressionDescription | string
OtherCompressionInfoDescription | string
OtherEnabledState | string
OtherErrorControlDescription | string
OtherErrorControlInfoDescription | string
OtherModulationDescription | string
OtherSchemeDescription | string
PowerManagementSupported | boolean
PowerOnHours | uint64
PrimaryStatus | uint16
RequestedState | uint16
RingsBeforeAnswer | uint8
SpeakerVolumeInfo | uint16
Status | string
StatusInfo | uint16
SupportsCallback | boolean
SupportsSynchronousConnect | boolean
SystemCreationClassName | string
SystemName | string
TimeOfLastReset | datetime
TimeOfLastStateChange | datetime
TotalPowerOnHours | uint64
TransitioningToState | uint16
AdditionalAvailability | uint16[]
AvailableRequestedStates | uint16[]
BlackListedNumbers | string[]
Capabilities | uint16[]
CapabilityDescriptions | string[]
CompressionSupported | uint16[]
CountriesSupported | string[]
CurrentPasswords | string[]
EnabledCapabilities | uint16[]
ErrorControlSupported | uint16[]
IdentifyingDescriptions | string[]
ModulationSupported | uint16[]
OperationalStatus | uint16[]
OtherIdentifyingInfo | string[]
PowerManagementCapabilities | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
EnableDevice | uint32
OnlineDevice | uint32
QuiesceDevice | uint32
RequestStateChange | uint32
Reset | uint32
RestoreProperties | uint32
SaveProperties | uint32
SetPowerState | uint32