# Class CIM_ATAProtocolEndpoint
extends CIM_ProtocolEndpoint

An ATAProtocolEndpoint represents the protocol (command) aspects of a logical ATA port, independent of the connection/transport. ATAProtocolEndpoint is either directly or indirectly associated to one or more instances of LogicalPort depending on the underlying transport.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_ServiceAccessPoint
|
+--CIM_ProtocolEndpoint
|
+--CIM_ATAProtocolEndpoint

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | An ATAProtocolEndpoint represents the protocol (command) aspects of a logical ATA port, independent of the connection/transport. ATAProtocolEndpoint is either directly or indirectly associated to one or more instances of LogicalPort depending on the underlying transport.
UMLPackagePath | string | CIM::Network::ProtocolEndpoints
Version | string | 2.45.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
ConnectionType | uint16 |
Description | string | The supported connection type for this endpoint. The connection type may be needed before the port(s) are associated and also is used in some ATA commands.
ValueMap | string | 1, 2, 3
Values | string | Other, ATA, SATA
Name | string |
Description | string | The ATA identifier for the target or initiator device, in the format appropriate for the ConnectionType. If a ConnectionType specific subclass is defined, the subclass may override Name to define the format. For other ConnectionTypes, the format (and content) should match that of PermanentAddress of the corresponding port if the port is is subclassed from NetworkPort.
Key | boolean | true
MaxLen | uint32 | 256
Override | string | Name
OtherConnectionType | string |
Description | string | The connection type, if ConnectionType is "Other".
Role | uint16 |
Description | string | This property indicates which role this ProtocolEndpoint implements.
ValueMap | string | 0, 2, 3, 4
Values | string | Unknown, Initiator, Target, Both Initiator and Target

### Inherited Properties

Name | Data Type
--- | ---
BroadcastResetSupported | boolean
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
NameFormat | string
OperatingStatus | uint16
OtherEnabledState | string
OtherTypeDescription | string
PrimaryStatus | uint16
ProtocolIFType | uint16
ProtocolType | uint16
RequestedState | uint16
Status | string
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TransitioningToState | uint16
AvailableRequestedStates | uint16[]
OperationalStatus | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
BroadcastReset | uint32
RequestStateChange | uint32