# Class CIM_PersistentMemoryNamespaceSettingData
extends CIM_ResourceAllocationSettingData

PersistentMemoryNamespaceSettingData reflects the parameters specified during persistent memory namespace creation or modification that define the quality of service offered by the associated PersistentMemoryNamespace.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_SettingData
|
+--CIM_ResourceAllocationSettingData
|
+--CIM_PersistentMemoryNamespaceSettingData

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | PersistentMemoryNamespaceSettingData reflects the parameters specified during persistent memory namespace creation or modification that define the quality of service offered by the associated PersistentMemoryNamespace.
UMLPackagePath | string | CIM::Device::ConfigurableMemory
Version | string | 2.47.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AccessType | uint16 |
Description | string | The type of access supported for the namespace."Read" read access is supported. "Write" write access is supported. "Read/Write" read and write access is supported.
ValueMap | string | 0, 2, 3, 4, .., 0x8000..0xFFFF
Values | string | Unknown, Read, Write, Read/Write, DMTF reserved, Vendor Reserved
Optimize | uint16 |
Description | string | Describes preferences relating to the allocation that can be described by flags "None" no specific optimizations requested. "Best Performance" Namespace optimized for best performance. "Smallest Size" Namespace optimized for smallest size. "Copy On Write" Namespace optimized for copy on write.
ValueMap | string | 0, 2, 3, 4, 5, .., 0x8000..0xFFFF
Values | string | Unknown, None, Best Performance, Smallest Size, Copy On Write, DMTF reserved, Vendor Reserved
ResourceType | uint16 |
Description | string | The type of resource this allocation setting represents. "Storage Volume" a logical block device. "Byte Addressable Persistent Memory" persistent memory accessible by load/store operations. "Block Addressable Persistent Memory" synthetic block device.
ModelCorrespondence | string | CIM_ResourceAllocationSettingData.OtherResourceType, CIM_ResourceAllocationSettingData.ResourceSubType
Override | string | ResourceType
ValueMap | string | 0, 1, 32, 35, 36, .., 0x8000..0xFFFF
Values | string | Unknown, Other, Storage Volume, Byte Addressable Persistent Memory, Block Addressable Persistent Memory, DMTF reserved, Vendor Reserved

### Inherited Properties

Name | Data Type
--- | ---
Address | string
AddressOnParent | string
AllocationUnits | string
AutomaticAllocation | boolean
AutomaticDeallocation | boolean
Caption | string
ChangeableType | uint16
ConfigurationName | string
ConsumerVisibility | uint16
Description | string
ElementName | string
Generation | uint64
InstanceID | string
Limit | uint64
MappingBehavior | uint16
OtherResourceType | string
Parent | string
PoolID | string
Reservation | uint64
ResourceSubType | string
SoID | string
SoOrgID | string
VirtualQuantity | uint64
VirtualQuantityUnits | string
Weight | uint32
ComponentSetting | string[]
Connection | string[]
HostResource | string[]

## Class Methods