# Class CIM_SCSIArbitraryLogicalUnit
extends CIM_LogicalDevice

SCSIArbitraryLogicalUnit represents an element that is addressed as a device, but is not accurately modeled by some other LogicalDevice subclass (such as TapeDrive or StorageVolume). One common use is 'control devices' that provide management rather than I/O functionality. For example, SCSI defines this behavior for Enclosure Services and SCSI Controller devices.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_SCSIArbitraryLogicalUnit

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | SCSIArbitraryLogicalUnit represents an element that is addressed as a device, but is not accurately modeled by some other LogicalDevice subclass (such as TapeDrive or StorageVolume). One common use is 'control devices' that provide management rather than I/O functionality. For example, SCSI defines this behavior for Enclosure Services and SCSI Controller devices.
UMLPackagePath | string | CIM::Device::DeviceElements
Version | string | 2.45.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
DeviceType | uint16 |
Description | string | The type of the device. For SCSI devices, this property is related to the peripheral device type that is returned in bits 0 to 4 of byte 0 of the inquiry response. Note that 'Direct Access' is included to model the common behavior of using a zero-length volume for in-band management of RAID arrays.
MappingStrings | string | ANSI|T10|SCSI SPC|Peripheral Device Type
ModelCorrespondence | string | CIM_SCSIArbitraryLogicalUnit.OtherDeviceType
Required | boolean | true
ValueMap | string | 0, 1, 2, 3, 4, 5, 6
Values | string | Unknown, Other, Direct Access, SCSI SCC Device, SCSI SES, SCSI ADI, SCSI Well Known Logical Unit
OtherDeviceType | string |
Description | string | A string that describes the device type if DeviceType is set to 1 ("Other").
ModelCorrespondence | string | CIM_SCSIArbitraryLogicalUnit.DeviceType

### Inherited Properties

Name | Data Type
--- | ---
AllocationState | string
Availability | uint16
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
DeviceID | string
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
ErrorCleared | boolean
ErrorDescription | string
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LastErrorCode | uint32
LocationIndicator | uint16
MaxQuiesceTime | uint64
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PowerManagementSupported | boolean
PowerOnHours | uint64
PrimaryStatus | uint16
RequestedState | uint16
Status | string
StatusInfo | uint16
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TotalPowerOnHours | uint64
TransitioningToState | uint16
AdditionalAvailability | uint16[]
AvailableRequestedStates | uint16[]
IdentifyingDescriptions | string[]
OperationalStatus | uint16[]
OtherIdentifyingInfo | string[]
PowerManagementCapabilities | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
EnableDevice | uint32
OnlineDevice | uint32
QuiesceDevice | uint32
RequestStateChange | uint32
Reset | uint32
RestoreProperties | uint32
SaveProperties | uint32
SetPowerState | uint32