# Class CIM_FCAdapterEventCounters
extends CIM_DeviceStatisticalInformation

Note: The use of the FCAdapterEventCounters class is deprecated because FibreChannelAdapter is deprecated. FCPortStatistics should be used instead, but it redefines the level at which data is collected. Therefore, there is no direct translation of the individual counters between the two classes. This object describes event counters that were specific to a FibreChannelAdapter.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_StatisticalInformation
|
+--CIM_DeviceStatisticalInformation
|
+--CIM_FCAdapterEventCounters

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Deprecated | string | CIM_FCPortStatistics
Description | string | Note: The use of the FCAdapterEventCounters class is deprecated because FibreChannelAdapter is deprecated. FCPortStatistics should be used instead, but it redefines the level at which data is collected. Therefore, there is no direct translation of the individual counters between the two classes. This object describes event counters that were specific to a FibreChannelAdapter.
UMLPackagePath | string | CIM::Device::NetworkAdapter
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
ABTSFramesReceived | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of Abort sequence frames received.
ABTSFramesRejected | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of Abort sequence frames sent where the response was BA_RJT.
ABTSFramesSent | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of Abort sequence frames sent.
FBSYsReceived | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of frames busied by the Fabric.
FRJTsReceived | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of frames rejected by the Fabric.
PBSYsReceived | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of frames busied by the receiving Node.
PBSYsSent | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of frames busied by the Adapter itself.
PRJTsReceived | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of frames rejected by the receiving Node.
PRJTsSent | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of frames rejected by the Adapter itself.
PRLIsRejected | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of PRLI frames sent where the response was LS_RJT.
PRLOsRejected | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of PRLO frames sent where the response was LS_RJT.

### Inherited Properties

Name | Data Type
--- | ---
Caption | string
CreationClassName | string
Description | string
DeviceCreationClassName | string
DeviceID | string
ElementName | string
Generation | uint64
InstanceID | string
Name | string
SystemCreationClassName | string
SystemName | string

## Class Methods