# Class CIM_FlatPanel
extends CIM_Display

Capabilities and management of the FlatPanel LogicalDevice.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_UserDevice
|
+--CIM_Display
|
+--CIM_FlatPanel

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Capabilities and management of the FlatPanel LogicalDevice.
UMLPackagePath | string | CIM::Device::UserDevices
Version | string | 2.23.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
DisplayType | uint16 |
Description | string | An integer enumeration describing the type of flat panel display.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8
Values | string | Unknown, Other, Passive Matrix LCD, Active Matrix LCD, Cholesteric LCD, Field Emission Display, Electro Luminescent Display, Gas Plasma, LED
HorizontalResolution | uint32 |
Description | string | FlatPanel's horizontal resolution in Pixels.
PUnit | string | pixel
Units | string | Pixels
LightSource | uint16 |
Description | string | A description of the display illumination type. For example, backlit (value=2) or reflective (4) can be specified.
ValueMap | string | 0, 1, 2, 3, 4
Values | string | Unknown, Other, Backlit, Edgelit, Reflective
ScanMode | uint16 |
Description | string | A FlatPanel's scan mode indicating either single (value=2) or dual scan (3).
ValueMap | string | 0, 1, 2, 3
Values | string | Unknown, Other, Single Scan, Dual Scan
SupportsColor | boolean |
Description | string | Boolean indicating whether the FlatPanel supports color display.
VerticalResolution | uint32 |
Description | string | FlatPanel's vertical resolution in Pixels.
PUnit | string | pixel
Units | string | Pixels

### Inherited Properties

Name | Data Type
--- | ---
AllocationState | string
Availability | uint16
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
DeviceID | string
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
ErrorCleared | boolean
ErrorDescription | string
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
IsLocked | boolean
LastErrorCode | uint32
LocationIndicator | uint16
MaxQuiesceTime | uint64
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PowerManagementSupported | boolean
PowerOnHours | uint64
PrimaryStatus | uint16
RequestedState | uint16
Status | string
StatusInfo | uint16
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TotalPowerOnHours | uint64
TransitioningToState | uint16
AdditionalAvailability | uint16[]
AvailableRequestedStates | uint16[]
IdentifyingDescriptions | string[]
OperationalStatus | uint16[]
OtherIdentifyingInfo | string[]
PowerManagementCapabilities | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
EnableDevice | uint32
OnlineDevice | uint32
QuiesceDevice | uint32
RequestStateChange | uint32
Reset | uint32
RestoreProperties | uint32
SaveProperties | uint32
SetPowerState | uint32