# Class CIM_MediaRedirectionSAP
extends CIM_ServiceAccessPoint

MediaRedirectionSAP is a logical representation of a Media redirection session. One access point represents access to a single Media redirection session.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_ServiceAccessPoint
|
+--CIM_MediaRedirectionSAP

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | MediaRedirectionSAP is a logical representation of a Media redirection session. One access point represents access to a single Media redirection session.
UMLPackagePath | string | CIM::Network::MediaRedirection
Version | string | 2.22.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
CommandTimeout | datetime |
Description | string | CommandTimeout is configurable by management applications supporting Media Redirections. When the Redirection Service redirects a Media device command to a remote device, and the remote device does not respond before CommandTimeout times out, the Redirection Service will emulate a media eject event and re-try the command and/or try to re-establish the connection to the remote device. Commandtimeout shall be expressed using the interval format of the datetime type.
ConnectionMode | uint16 |
Description | string | An enumeration specifying the type of connection mode supported by the session. A value set to 2 = "Listen" shall indicate that the SAP will listen for a connection request from the remote Media redirection server. A CIM_BindsTo association to a CIM_ProtocolEndpoint may be used to represent where the SAP is listening for the connection request. A value set to 3 = "Connect" shall indicate that the the SAP shall initiate the connection to the remote Media redirection server. A CIM_RemoteAccessAvailableToElement association to a CIM_RemoteServiceAccessPoint may be used to represent where the SAP shall connect to the remote Media redirection server.
ValueMap | string | 0, 2, 3, .., 32768..65535
Values | string | Unknown, Listen, Connect, DMTF Reserved, Vendor Specified
ResetTimeout | datetime |
Description | string | The amount of time the session shall wait after sending a Reset to the Remote System before concluding that the Remote System is not responding in a timely fashion, it may be hung or busy. When the Reset Timeout is exceeded the managed system tries to establish a new connection with the Remote System. ResetTimeout shall be expressed using the interval format of the datetime type.
SessionTimeout | datetime |
Description | string | The amount of time the session will wait for a Remote System to establish a new connection before the Media Device is detached. SessionTimeout shall be expressed using the interval format of the datetime type.

### Inherited Properties

Name | Data Type
--- | ---
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PrimaryStatus | uint16
RequestedState | uint16
Status | string
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TransitioningToState | uint16
AvailableRequestedStates | uint16[]
OperationalStatus | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
RequestStateChange | uint32