# Class CIM_LabelReader
extends CIM_LogicalDevice

LabelReaders represent hardware capable of scanning or reading a physical label or the NonVolatileMemory on a PhysicalMedia. Examples of labels include barcode and OCR tags.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_LabelReader

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | LabelReaders represent hardware capable of scanning or reading a physical label or the NonVolatileMemory on a PhysicalMedia. Examples of labels include barcode and OCR tags.
UMLPackagePath | string | CIM::Device::StorageLib
Version | string | 2.6.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
Technology | uint16 |
Description | string | The technology used by the LabelReader. One entry of the Values array requires some explanation - "Memory Reader". The latter describes the ability to access memory in a PhysicalMedia's packaging (for example, memory on an AIT tape). The existence of this Memory is indicated by the MemoryWithMedia association on the physical side, or by AssociatedMemory on the logical side.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6
Values | string | Unknown, Other, Laser, Infrared, RF, Camera, Memory Reader
SupportedFormats | uint16[] |
Description | string | An array of enumerated integers describing the formats of the labels that can be read or scanned by the LabelReader. The values specified for this property correspond to those defined for CIM_PhysicalMedia.LabelFormats.
ModelCorrespondence | string | CIM_PhysicalMedia.LabelFormats
ValueMap | string | 0, 1, 2, 3, 4, 5
Values | string | Barcode, Radio Frequency Identification, OCR (Optical Character Recognition), MICR (Magnetic Ink Character Recognition), 7 Character Barcode, 9 Character Barcode

### Inherited Properties

Name | Data Type
--- | ---
AllocationState | string
Availability | uint16
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
DeviceID | string
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
ErrorCleared | boolean
ErrorDescription | string
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LastErrorCode | uint32
LocationIndicator | uint16
MaxQuiesceTime | uint64
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PowerManagementSupported | boolean
PowerOnHours | uint64
PrimaryStatus | uint16
RequestedState | uint16
Status | string
StatusInfo | uint16
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TotalPowerOnHours | uint64
TransitioningToState | uint16
AdditionalAvailability | uint16[]
AvailableRequestedStates | uint16[]
IdentifyingDescriptions | string[]
OperationalStatus | uint16[]
OtherIdentifyingInfo | string[]
PowerManagementCapabilities | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
EnableDevice | uint32
OnlineDevice | uint32
QuiesceDevice | uint32
RequestStateChange | uint32
Reset | uint32
RestoreProperties | uint32
SaveProperties | uint32
SetPowerState | uint32