# Class CIM_PhysicalFrame
extends CIM_PhysicalPackage

PhysicalFrame is a superclass of Rack, Chassis and other frame enclosures, as they are defined in extension classes. Properties like visible or audible alarm, and data related to security breaches are in this superclass.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_PhysicalElement
|
+--CIM_PhysicalPackage
|
+--CIM_PhysicalFrame

## Direct Known Subclasses

CIM_Chassis
CIM_Rack

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | PhysicalFrame is a superclass of Rack, Chassis and other frame enclosures, as they are defined in extension classes. Properties like visible or audible alarm, and data related to security breaches are in this superclass.
UMLPackagePath | string | CIM::Physical::Package
Version | string | 2.7.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AudibleAlarm | boolean |
Description | string | Boolean indicating whether the Frame is equipped with an audible alarm.
BreachDescription | string |
Description | string | BreachDescription is a free-form string providing more information if the SecurityBreach property indicates that a breach or some other security-related event occurred.
ModelCorrespondence | string | CIM_PhysicalFrame.SecurityBreach
CableManagementStrategy | string |
Description | string | CableManagementStrategy is a free-form string that contains information on how the various cables are connected and bundled for the Frame. With many networking, storage-related and power cables, cable management can be a complex and challenging endeavor. This string property contains information to aid in assembly and service of the Frame.
IsLocked | boolean |
Description | string | Boolean indicating that the Frame is currently locked.
LockPresent | boolean |
Description | string | Boolean indicating whether the Frame is protected with a lock.
SecurityBreach | uint16 |
Description | string | SecurityBreach is an enumerated, integer-valued property indicating whether a physical breach of the Frame was attempted but unsuccessful (value=4) or attempted and successful (5). Also, the values, "Unknown", "Other" or "No Breach", can be specified.
MappingStrings | string | MIF.DMTF|Physical Container Global Table|004.12
ModelCorrespondence | string | CIM_PhysicalFrame.BreachDescription
ValueMap | string | 1, 2, 3, 4, 5
Values | string | Other, Unknown, No Breach, Breach Attempted, Breach Successful
VisibleAlarm | boolean |
Description | string | Boolean indicating that the equipment includes a visible alarm.
ServiceDescriptions | string[] |
ArrayType | string | Indexed
Description | string | An array of free-form strings providing more detailed explanations for any of the entries in the Service Philosophy array. Note, each entry of this array is related to the entry in ServicePhilosophy that is located at the same index.
ModelCorrespondence | string | CIM_PhysicalFrame.ServicePhilosophy
ServicePhilosophy | uint16[] |
ArrayType | string | Indexed
Description | string | ServicePhilosophy is an enumerated, integer-valued array that indicates whether the Frame is serviced from the top (value=2), front (3), back (4) or side (5), whether it has sliding trays (6) or removable sides (7), and/or whether the Frame is moveable (8), for example, having rollers.
ModelCorrespondence | string | CIM_PhysicalFrame.ServiceDescriptions
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8
Values | string | Unknown, Other, Service From Top, Service From Front, Service From Back, Service From Side, Sliding Trays, Removable Sides, Moveable

### Inherited Properties

Name | Data Type
--- | ---
CanBeFRUed | boolean
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Depth | real32
Description | string
DetailedStatus | uint16
ElementName | string
Generation | uint64
HealthState | uint16
Height | real32
HotSwappable | boolean
InstallDate | datetime
InstanceID | string
ManufactureDate | datetime
Manufacturer | string
Model | string
Name | string
OperatingStatus | uint16
OtherIdentifyingInfo | string
OtherPackageType | string
PackageType | uint16
PartNumber | string
PoweredOn | boolean
PrimaryStatus | uint16
Removable | boolean
RemovalConditions | uint16
Replaceable | boolean
SerialNumber | string
SKU | string
Status | string
Tag | string
UserTracking | string
VendorEquipmentType | string
Version | string
Weight | real32
Width | real32
OperationalStatus | uint16[]
StatusDescriptions | string[]
VendorCompatibilityStrings | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
IsCompatible | uint32