# Class CIM_FibrePortEventCounters
extends CIM_DeviceStatisticalInformation

Note: The use of the FibrePortEventCounters class is deprecated because FibrePort is deprecated. FCPortStatistics should be used instead, but it redefines the level at which data is collected. Therefore, there is no direct translation of the individual counters between the two classes. Deprecated description: This object defines error counters that are specific to a FibrePort.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_StatisticalInformation
|
+--CIM_DeviceStatisticalInformation
|
+--CIM_FibrePortEventCounters

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Deprecated | string | CIM_FCPortStatistics
Description | string | Note: The use of the FibrePortEventCounters class is deprecated because FibrePort is deprecated. FCPortStatistics should be used instead, but it redefines the level at which data is collected. Therefore, there is no direct translation of the individual counters between the two classes. Deprecated description: This object defines error counters that are specific to a FibrePort.
UMLPackagePath | string | CIM::Device::NetworkAdapter
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
EOFAbortsReceived | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: Number of frames received that contain 'EOF Abort'.
EOFAbortsTransmitted | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: Number of frames transmitted that contain 'EOF Abort'.
PLOGIsReceived | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of login frames received.
PLOGIsRejected | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of PLOGI frames sent where the response was LS_RJT.
PLOGIsSent | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of login frames sent.
PLOGOsReceived | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of logouts that were received from various targets.
PLOGOsRejected | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of PLOGO frames sent where the response was LS_RJT.
PLOGOsSent | uint64 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The number of logout frames sent.

### Inherited Properties

Name | Data Type
--- | ---
Caption | string
CreationClassName | string
Description | string
DeviceCreationClassName | string
DeviceID | string
ElementName | string
Generation | uint64
InstanceID | string
Name | string
SystemCreationClassName | string
SystemName | string

## Class Methods