# Class CIM_InitiatorTargetLogicalUnitPath

An association that models a host driver path to a logical unit. Each permutation of initiator and target ProtocolEndpoints and logical units is considered a separate path.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_InitiatorTargetLogicalUnitPath

## Direct Known Subclasses

CIM_ATAInitiatorTargetLogicalUnitPath
CIM_SCSIInitiatorTargetLogicalUnitPath

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Association | boolean | true
Description | string | An association that models a host driver path to a logical unit. Each permutation of initiator and target ProtocolEndpoints and logical units is considered a separate path.
UMLPackagePath | string | CIM::Device::StorageDevices
Version | string | 2.45.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
State | uint32 |
Description | string | The state of this path. Values are defined as follows: Unknown - the path is unavailable,but the cause is not known. Active - The path is okay and active. Passive - The path is okay, but is associated with a target port of target port group in standby access state. Only applies to devices with asymmetric access. Disabled - The path is disabled by administrative request (DisablePathLU). Path Error - The path is unusable due to an error on this path and no SCSI status was received. Logical Unit Error - A SCSI status was received for an I/O through this path indicating a logical unit error. Reserved - The path is unavailable due to a reservation. Removed - The path is unavailable because the OS or drivers marked the pathunusable. Transitioning - the path is transitioning between two valid states. The only valid values a client can specify are Disabled and Active. All other states are determined by the underlying implementation; attempts to set them should be given an error response.
MappingStrings | string | MP_API.SNIA|MP_PATH_LOGICAL_UNIT_PROPERTIES|pathState
ValueMap | string | 0, 2, 3, 4, 5, 6, 7, 8, 9
Values | string | Unknown, Active, Passive, Disabled, Path Error, Logical Unit Error, Reserved, Removed, Transitioning
Write | boolean | true

### Association References

Name | Reference Class
--- | ---
Initiator | CIM_ProtocolEndpoint
LogicalUnit | CIM_LogicalDevice
Target | CIM_ProtocolEndpoint

## Class Methods