# Class CIM_PowerUtilizationManagementService
extends CIM_Service

PowerUtilizationManagementService represents the ability of a platform or component to perform autonomic management of its power utilization.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_PowerUtilizationManagementService

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | PowerUtilizationManagementService represents the ability of a platform or component to perform autonomic management of its power utilization.
UMLPackagePath | string | CIM::Device::CoolingAndPower
Version | string | 2.23.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
PowerUtilizationMode | uint16 | 2
Description | string | PowerUtilizationMode indicates the current power utilization mode implemented by the service. The mode selection is a generally made infrequently as part of element configuration. A value of "None" shall indicate that no effort is being made to reduce the power consumed by the system below nominal. A value of "Dynamic" shall indicate the PowerUtilizationManagementService is actively modifying the configuration of one or more system components in order to reduce the power consumed. A value of "Static" shall indicate the system whose power utilization functionality is represented by the PowerUtilizationManagementService is operating with a fixed configuration resulting in a lower level of power consumption than nominal. Static mode differs from dynamic in that the mode corresponds to a single fixed configuration, while dynamic mode implies frequent changes in system configuration.
ModelCorrespondence | string | CIM_PowerUtilizationManagementCapabilities.PowerUtilizationModesSupported
ValueMap | string | 2, 3, 4, .., 32768..65535
Values | string | None, Dynamic, Static, DMTF Reserved, Vendor Reserved

### Inherited Properties

Name | Data Type
--- | ---
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LoSID | string
LoSOrgID | string
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PrimaryOwnerContact | string
PrimaryOwnerName | string
PrimaryStatus | uint16
RequestedState | uint16
Started | boolean
StartMode | string
Status | string
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TransitioningToState | uint16
AvailableRequestedStates | uint16[]
OperationalStatus | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
ChangeAffectedElementsAssignedSequence | uint32
RequestStateChange | uint32
StartService | uint32
StopService | uint32