# Class CIM_DSCPMarkerService
extends CIM_MarkerService

DSCPMarkerService marks the differentiated services codepoint (DSCP) within the DS field in the IPv4 and IPv6 packet headers, as defined in [R2474]. It is marked with the specific value defined in the property, DSCPValue. Following common practice, the value to be written into the field is represented as an unsigned 8-bit integer.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_ConditioningService
|
+--CIM_MarkerService
|
+--CIM_DSCPMarkerService

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | DSCPMarkerService marks the differentiated services codepoint (DSCP) within the DS field in the IPv4 and IPv6 packet headers, as defined in [R2474]. It is marked with the specific value defined in the property, DSCPValue. Following common practice, the value to be written into the field is represented as an unsigned 8-bit integer.
UMLPackagePath | string | CIM::Network::QoS
Version | string | 2.7.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
DSCPValue | uint8 |
Description | string | This property is an unsigned 8-bit integer, representing a value to be used for marking the DSCP field in an IPv4 or Ipv6 packet header. Since the DSCP consists of 6 bits, the values for this property are limited to the range 0..63. When the DSCP is marked, the remaining two bits in the DS field are left unchanged.
MaxValue | sint64 | 63
MinValue | sint64 | 0

### Inherited Properties

Name | Data Type
--- | ---
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
ElementName | string
Enabled | boolean
EnabledDefault | uint16
EnabledState | uint16
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LoSID | string
LoSOrgID | string
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PrimaryOwnerContact | string
PrimaryOwnerName | string
PrimaryStatus | uint16
RequestedState | uint16
Started | boolean
StartMode | string
Status | string
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TransitioningToState | uint16
AvailableRequestedStates | uint16[]
OperationalStatus | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
ChangeAffectedElementsAssignedSequence | uint32
RequestStateChange | uint32
StartService | uint32
StopService | uint32