# Class CIM_SystemBusCard
extends CIM_Card

The SystemBusCard class represents additional information for a CIM_Card, detailing the Card's bus type and data width. These properties dictate the type of Slot into which the Card can be inserted. For example, using the properties of this class, one can define that a Card is a PCI, 64 bit adapter.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_PhysicalElement
|
+--CIM_PhysicalPackage
|
+--CIM_Card
|
+--CIM_SystemBusCard

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | The SystemBusCard class represents additional information for a CIM_Card, detailing the Card's bus type and data width. These properties dictate the type of Slot into which the Card can be inserted. For example, using the properties of this class, one can define that a Card is a PCI, 64 bit adapter.
UMLPackagePath | string | CIM::Physical::Package
Version | string | 2.19.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
BusType | uint16 |
Description | string | An enumerated integer describing the System bus type for this Card. It indicates the type of Slot into which the Card can plug. The list of permissible values aligns with the System bus types in CIM_PhysicalConnector.Connector Type.
ModelCorrespondence | string | CIM_PhysicalConnector.ConnectorType
ValueMap | string | 43, 44, 45, 46, 47, 48, 49, 50, 52, 64, 65, 73, 74, 75, 76, 77, 78, 79, 80, 81, 82, 83, 84, 85, 86, 87, 98, 99, 100, 101, 102, 103, 104, 105, 106, 109, 110, 111, 112
Values | string | PCI, ISA, EISA, VESA, PCMCIA, PCMCIA Type I, PCMCIA Type II, PCMCIA Type III, CardBus, Access.bus, NuBus, AGP, VME Bus, VME64, Proprietary, Proprietary Processor Card Slot, Proprietary Memory Card Slot, Proprietary I/O Riser Slot, PCI-66MHZ, AGP2X, AGP4X, PC-98, PC-98-Hireso, PC-H98, PC-98Note, PC-98Full, PCI-X, Sbus IEEE 1396-1993 32 bit, Sbus IEEE 1396-1993 64 bit, MCA, GIO, XIO, HIO, NGIO, PMC, Future I/O, InfiniBand, AGP8X, PCI-E
BusWidth | uint16 |
Description | string | System bus width (in bits) required by this Card. If 'unknown', enter 0. If 'other' than the values, 8, 16, 32, 64 or 128, enter 1. The list of permissible values aligns with the data in CIM_Slot.MaxBusWidth.
ModelCorrespondence | string | CIM_Slot.MaxDataWidth
PUnit | string | bit
Units | string | Bits
ValueMap | string | 0, 1, 8, 16, 32, 64, 128

### Inherited Properties

Name | Data Type
--- | ---
CanBeFRUed | boolean
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Depth | real32
Description | string
DetailedStatus | uint16
ElementName | string
Generation | uint64
HealthState | uint16
Height | real32
HostingBoard | boolean
HotSwappable | boolean
InstallDate | datetime
InstanceID | string
ManufactureDate | datetime
Manufacturer | string
Model | string
Name | string
OperatingStatus | uint16
OtherIdentifyingInfo | string
OtherPackageType | string
PackageType | uint16
PartNumber | string
PoweredOn | boolean
PrimaryStatus | uint16
Removable | boolean
RemovalConditions | uint16
Replaceable | boolean
RequirementsDescription | string
RequiresDaughterBoard | boolean
SerialNumber | string
SKU | string
SlotLayout | string
SpecialRequirements | boolean
Status | string
Tag | string
UserTracking | string
VendorEquipmentType | string
Version | string
Weight | real32
Width | real32
OperatingVoltages | sint16[]
OperationalStatus | uint16[]
StatusDescriptions | string[]
VendorCompatibilityStrings | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
ConnectorPower | uint32
IsCompatible | uint32