# Class CIM_SATransform
extends CIM_ScopedSettingData

SATransform is the base class for the various types of transforms that are in effect for an existing IPsecSAEndpoint, or aggregated into phase 2 proposals used during the IPsec negotiation process. This class is defined as a kind of ScopedSettingData, since it describes the set of transform properties that MUST be applied together, if negotiated. This subclassing is different than that defined in IETF's IPSP Policy draft - where it is subclassed from Policy. The definition as SettingData is more consistent with the application of the properties as a set, to the negotiated Security Association. Note that an instance of this class is 'scoped' or contained by a System (either a ComputerSystem or AdminDomain), rather than by a SecurityAssociationEndpoint. This is indicated by instantiating the ScopedSetting association, and is necessary since the transform data is used in IPsec negotiation policies (also scoped by Systems) before ever being associated with a SecurityAssociationEndpoint. The latter semantics (i.e., that 'this' transform is negotiated for 'this' Security Association) is conveyed via a subclass of ElementSettingData, TransformOfSecurityAssociation.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_SettingData
|
+--CIM_ScopedSettingData
|
+--CIM_SATransform

## Direct Known Subclasses

CIM_AHTransform
CIM_ESPTransform
CIM_IPCOMPTransform

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Abstract | boolean | true
Description | string | SATransform is the base class for the various types of transforms that are in effect for an existing IPsecSAEndpoint, or aggregated into phase 2 proposals used during the IPsec negotiation process. This class is defined as a kind of ScopedSettingData, since it describes the set of transform properties that MUST be applied together, if negotiated. This subclassing is different than that defined in IETF's IPSP Policy draft - where it is subclassed from Policy. The definition as SettingData is more consistent with the application of the properties as a set, to the negotiated Security Association. Note that an instance of this class is 'scoped' or contained by a System (either a ComputerSystem or AdminDomain), rather than by a SecurityAssociationEndpoint. This is indicated by instantiating the ScopedSetting association, and is necessary since the transform data is used in IPsec negotiation policies (also scoped by Systems) before ever being associated with a SecurityAssociationEndpoint. The latter semantics (i.e., that 'this' transform is negotiated for 'this' Security Association) is conveyed via a subclass of ElementSettingData, TransformOfSecurityAssociation.
MappingStrings | string | IPSP Model.IETF|SATransform
UMLPackagePath | string | CIM::Network::IPsec
Version | string | 2.8.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
ElementName | string |
Description | string | The user-friendly name for this instance of SettingData. In addition, the user-friendly name can be used as an index property for a search or query. (Note: The name does not have to be unique within a namespace.)
MappingStrings | string | IPSP Model.IETF|SATransform.CommonName
Override | string | ElementName
Required | boolean | true
MaxLifetimeKilobytes | uint64 | 0
Description | string | MaxLifetimeKilobytes specifies the maximum kilobyte lifetime for a Security Association. Different lifetimes are used, depending on the strength of the encryption algorithm. A value of 0, the default, indicates that no maximum should be defined. A non-zero value specifies the desired kilobyte lifetime.
MappingStrings | string | IPSP Model.IETF|SATransform.MaxLifetimeKilobytes
PUnit | string | byte * 10^3
Units | string | KiloBytes
MaxLifetimeSeconds | uint64 | 0
Description | string | MaxLifetimeSeconds specifies the maximum time that the Security Association should be considered valid after it has been created. A value of 0, the default, indicates that 8 hours should be used. A non-zero value indicates the maximum lifetime in seconds.
MappingStrings | string | IPSP Model.IETF|SATransform.MaxLifetimeSeconds
PUnit | string | second
Units | string | Seconds
VendorID | string |
Description | string | VendorID identifies vendor-defined transforms. If this field is empty (the default), then this is a standard transform.
MappingStrings | string | IPSP Model.IETF|SATransform.VendorID

### Inherited Properties

Name | Data Type
--- | ---
Caption | string
ChangeableType | uint16
ConfigurationName | string
Description | string
Generation | uint64
InstanceID | string
SoID | string
SoOrgID | string
ComponentSetting | string[]

## Class Methods