# Class CIM_SCSIController
extends CIM_Controller

Note: The use of this class is deprecated in lieu of SCSIProtocolController. The latter reflects the protocol- related issues of SCSI interfaces, because these are not bus master-type Controllers." Deprecated description: Capabilities and management of the SCSIController.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_Controller
|
+--CIM_SCSIController

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Deprecated | string | CIM_SCSIProtocolController
Description | string | Note: The use of this class is deprecated in lieu of SCSIProtocolController. The latter reflects the protocol- related issues of SCSI interfaces, because these are not bus master-type Controllers." Deprecated description: Capabilities and management of the SCSIController.
UMLPackagePath | string | CIM::Device::Controller
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
ControllerTimeouts | uint32 |
Counter | boolean | true
Deprecated | string | No value
Description | string | Note: The use of this method is deprecated. Deprecated description: Number of SCSIController timeouts that have occurred since the TimeOfLastReset.
MaxDataWidth | uint32 |
Deprecated | string | No value
Description | string | Note: The use of this method is deprecated. Deprecated description: Maximum data width (in bits) supported by the SCSIController.
MappingStrings | string | MIF.DMTF|Bus Port|004.7
PUnit | string | bit
Units | string | Bits
MaxTransferRate | uint64 |
Deprecated | string | No value
Description | string | Note: The use of this method is deprecated. Deprecated description: Maximum transfer rate (in Bits per Second) supported by the SCSIController.
MappingStrings | string | MIF.DMTF|Bus Port|004.8
PUnit | string | bit / second
Units | string | Bits per Second
ProtectionManagement | uint16 |
Deprecated | string | No value
Description | string | Note: The use of this method is deprecated. Deprecated description: An integer enumeration that indicates whether or not the SCSIController provides redundancy or protection against device failures.
MappingStrings | string | MIF.DMTF|Storage Controller|001.3
ValueMap | string | 1, 2, 3, 4, 5, 6
Values | string | Other, Unknown, Unprotected, Protected, Protected through SCC (SCSI-3 Controller Command), Protected through SCC-2 (SCSI-3 Controller Command)
SignalCapabilities | uint16[] |
Deprecated | string | No value
Description | string | Note: The use of this method is deprecated. Deprecated description: Signal capabilities that can be supported by the SCSIController. For example, the Controller can support "Single Ended" and "Differential". In this case, the values 3 and 4 would be written to the Signal Capabilities array.
ModelCorrespondence | string | CIM_SCSIInterface.SCSISignal
ValueMap | string | 1, 2, 3, 4, 5, 6
Values | string | Other, Unknown, Single Ended, Differential, Low Voltage Differential, Optical

### Inherited Properties

Name | Data Type
--- | ---
AllocationState | string
Availability | uint16
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
DeviceID | string
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
ErrorCleared | boolean
ErrorDescription | string
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LastErrorCode | uint32
LocationIndicator | uint16
MaxNumberControlled | uint32
MaxQuiesceTime | uint64
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PowerManagementSupported | boolean
PowerOnHours | uint64
PrimaryStatus | uint16
ProtocolDescription | string
ProtocolSupported | uint16
RequestedState | uint16
Status | string
StatusInfo | uint16
SystemCreationClassName | string
SystemName | string
TimeOfLastReset | datetime
TimeOfLastStateChange | datetime
TotalPowerOnHours | uint64
TransitioningToState | uint16
AdditionalAvailability | uint16[]
AvailableRequestedStates | uint16[]
IdentifyingDescriptions | string[]
OperationalStatus | uint16[]
OtherIdentifyingInfo | string[]
PowerManagementCapabilities | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
EnableDevice | uint32
OnlineDevice | uint32
QuiesceDevice | uint32
RequestStateChange | uint32
Reset | uint32
RestoreProperties | uint32
SaveProperties | uint32
SetPowerState | uint32