# Class CIM_IndicatorLED
extends CIM_LogicalDevice

CIM_IndicatorLED represents an LED of a managed element used to indicate one or more conditions for the managed element. A single discrete package may be represented by one or more instances of CIM_IndicatorLED. There may be an instance of CIM_IndicatorLED for each IndicatedCondition that may be indicated simultaneously by the discrete package. For example, if a single LED is capable of flashing yellow for one condition and blue for a different one, but the conditions are not indicated simultaneously, it is modeled using a single instance of CIM_IndicatorLED that supports both colors. If the LED indicated both conditions simultaneously, i.e. the package was lit yellow and blue simultaneously, there would be two instances of CIM_IndicatorLED.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_IndicatorLED

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | CIM_IndicatorLED represents an LED of a managed element used to indicate one or more conditions for the managed element. A single discrete package may be represented by one or more instances of CIM_IndicatorLED. There may be an instance of CIM_IndicatorLED for each IndicatedCondition that may be indicated simultaneously by the discrete package. For example, if a single LED is capable of flashing yellow for one condition and blue for a different one, but the conditions are not indicated simultaneously, it is modeled using a single instance of CIM_IndicatorLED that supports both colors. If the LED indicated both conditions simultaneously, i.e. the package was lit yellow and blue simultaneously, there would be two instances of CIM_IndicatorLED.
UMLPackagePath | string | CIM::Device::Sensors
Version | string | 2.39.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
ActivationState | uint16 |
Description | string | ActivationState indicates the current activity of an LED. An LED may exhibit behaviors that vary greatly in complexity. If the behavior of the LED is simple or a detailed depiction of the behavior is unnecessary to convey to client applications, values of than 5 "ControlPattern" may be used to indicate the behavior. If the behavior is complex and detailed information about the behavior is meaningful to a client, the value 5 "ControlPattern" shall be used to indicate the ControlPattern property describes the behavior. 2 "Lit" shall indicate the LED is continuously illuminated without variation in color or intensity. 3 "Blinking" shall indicate the LED is alternating between illuminated and not illuminated in a regular pattern without variation in color or intensity. The pattern is not indicated. 4 "Off" shall indicate the LED is not illuminated. 5 "ControlPattern" shall indicate the LED is exhibiting behavior that is described using the ControlPattern property.
ModelCorrespondence | string | CIM_IndicatorLED.ControlPattern, CIM_IndicatorLEDCapabilities.SupportedActivationStates
ValueMap | string | 0, 2, 3, 4, 5, .., 32768..65535
Values | string | Unknown, Lit, Blinking, Off, Control Pattern, DMTF Reserved, Vendor Reserved
Write | boolean | true
Color | uint16 |
Description | string | This property shall indicate the current color of the LED. If the value of the ActivationState property is 4 "Off" this property shall indicate the color of the LED the last time it was lit, or shall have the value 2 "Not Applicable".
ModelCorrespondence | string | CIM_IndicatorLED.OtherColorDescription, CIM_IndicatorLEDCapabilities.SupportedColors
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, .., 32768..65535
Values | string | Unknown, Other, Not Applicable, White, Red, Green, Blue, Orange, Yellow, Black, DMTF Reserved, Vendor Reserved
Write | boolean | true
ControlMode | uint16 |
Description | string | ControlMode indicates the current control mode for the LED.2 "Automatic" shall indicate the state of the LED is being controlled by the management infrastructure. 3 "Manual" shall indicate the state of the LED is being controlled by a management client. 4 "Test" shall indicate the LED is in a test mode.
ModelCorrespondence | string | CIM_IndicatorLEDCapabilities.SupportedControlModes
ValueMap | string | 2, 3, 4, .., 32768..65535
Values | string | Automatic, Manual, Test, DMTF Reserved, Vendor Reserved
Write | boolean | true
ControlPattern | string |
Description | string | An LED may exhibit a range of behavior from very simple (ex. solid on) to very complicated (ex. a series of blinks of alternating color and duration). ControlPattern specifies the vendor or standard behavior exhibited by the LED if it cannot be described using one of the standard behaviors listed for the ActivationState property. If ActivationState has the value 5 "ControlPattern", the ControlPattern property shall not be NULL. The value of ControlPattern shall be constructed using the following "preferred" algorithm: <OrgID>::<Pattern> Where <OrgID> and < Pattern> are separated by two colons (::), and where <OrgID> shall include a copyrighted, trademarked, or otherwise unique name that is owned by the business entity that is creating or defining the ControlPattern or that is a registered ID assigned to the business entity by a recognized global authority. If the definition of the value is specified by the DMTF, the value of <OrgID> shall be "DMTF". <Pattern> is chosen by the business entity and shall not be reused to identify different underlying (real-world) behaviors. If the behavior specified for the LED adheres to a standard or proprietary specification, <Pattern> shall be a uniquely assigned value identifying the behavior. If the behavior for the LED is described using a standard or proprietary grammar, <Pattern> shall be prefixed with a uniquely assigned identifier for the grammar.
ModelCorrespondence | string | CIM_IndicatorLED.ActivationState, CIM_IndicatorLEDCapabilities.SupportedControlPatterns
Write | boolean | true
DefaultActivationState | uint16 |
Description | string | DefaultActivationState indicates the default state of an LED. See ActivationState for a description of the values.
ValueMap | string | 0, 2, 3, 4, 5, .., 32768..65535
Values | string | Unknown, Lit, Blinking, Off, Control Pattern, DMTF Reserved, Vendor Reserved
OtherColorDescription | string |
Description | string | This property shall have a value if Color contains the value 1 "Other".
ModelCorrespondence | string | CIM_IndicatorLED.Color, CIM_IndicatorLEDCapabilities.OtherSupportedColorDescriptions
Write | boolean | true
OtherIndicatedConditionDescription | string |
Description | string | This property shall have a value if IndicatedConditions contains the value 1 "Other".
ModelCorrespondence | string | CIM_IndicatorLED.IndicatedConditions
IndicatedConditions | uint16[] |
Description | string | The condition indicated by the LED. 2 "Not Applicable" shall indicate the LED is currently not assigned an interpretation. 3 "Location" shall indicate the location of associated managed elements. 4 "Attention" shall indicate that the associated managed elements requires the attention of service personnel. 5 "Activity" shall indicate that activity is occurring for the associated managed elements. The type of activity indicated is specific to the associated managed elements. 6 "Powered On" shall indicate that the associated managed elements are receiving power. 7 "Fault" shall indicate that the associated managed elements are in a fault, error, or otherwise degraded state.
ModelCorrespondence | string | CIM_IndicatorLED.OtherIndicatedConditionDescription
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, .., 32768..65535
Values | string | Unknown, Other, Not Applicable, Location, Attention, Activity, Powered On, Fault, DMTF Reserved, Vendor Reserved

### Inherited Properties

Name | Data Type
--- | ---
AllocationState | string
Availability | uint16
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
DeviceID | string
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
ErrorCleared | boolean
ErrorDescription | string
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LastErrorCode | uint32
LocationIndicator | uint16
MaxQuiesceTime | uint64
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PowerManagementSupported | boolean
PowerOnHours | uint64
PrimaryStatus | uint16
RequestedState | uint16
Status | string
StatusInfo | uint16
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TotalPowerOnHours | uint64
TransitioningToState | uint16
AdditionalAvailability | uint16[]
AvailableRequestedStates | uint16[]
IdentifyingDescriptions | string[]
OperationalStatus | uint16[]
OtherIdentifyingInfo | string[]
PowerManagementCapabilities | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
EnableDevice | uint32
OnlineDevice | uint32
QuiesceDevice | uint32
RequestStateChange | uint32
Reset | uint32
RestoreProperties | uint32
SaveProperties | uint32
SetPowerState | uint32