# Class CIM_SerialController
extends CIM_Controller

Capabilities and management of the SerialController.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_Controller
|
+--CIM_SerialController

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Capabilities and management of the SerialController.
UMLPackagePath | string | CIM::Device::Controller
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
MaxBaudRate | uint32 |
Description | string | Maximum baud rate in Bits per Second that is supported by the SerialController.
MappingStrings | string | MIF.DMTF|Serial Ports|004.6
PUnit | string | bit / second
Units | string | Bits per Second
Security | uint16 |
Description | string | An enumeration that indicates the operational security for the Controller. For example, information that the external interface of the Device is locked out (value=4) or "Boot Bypass" (value=6) can be described using this property.
MappingStrings | string | MIF.DMTF|Serial Ports|004.9
ValueMap | string | 1, 2, 3, 4, 5, 6
Values | string | Other, Unknown, None, External Interface Locked Out, External Interface Enabled, Boot Bypass
Capabilities | uint16[] |
ArrayType | string | Indexed
Description | string | The Capabilities property defines chip level compatibility for the SerialController. Therefore, this property describes the buffering and other capabilities of the SerialController that might be inherent in the chip hardware. The property is an enumerated integer.
MappingStrings | string | MIF.DMTF|Serial Ports|004.7
ModelCorrespondence | string | CIM_SerialController.CapabilityDescriptions
ValueMap | string | 1, 2, 3, 4, 5, 6, 160, 161
Values | string | Other, Unknown, XT/AT Compatible, 16450 Compatible, 16550 Compatible, 16550A Compatible, 8251 Compatible, 8251FIFO Compatible
CapabilityDescriptions | string[] |
ArrayType | string | Indexed
Description | string | An array of free-form strings that provides more detailed explanations for any of the SerialController features that are indicated in the Capabilities array. Note, each entry of this array is related to the entry in the Capabilities array that is located at the same index.
ModelCorrespondence | string | CIM_SerialController.Capabilities

### Inherited Properties

Name | Data Type
--- | ---
AllocationState | string
Availability | uint16
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
DeviceID | string
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
ErrorCleared | boolean
ErrorDescription | string
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LastErrorCode | uint32
LocationIndicator | uint16
MaxNumberControlled | uint32
MaxQuiesceTime | uint64
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PowerManagementSupported | boolean
PowerOnHours | uint64
PrimaryStatus | uint16
ProtocolDescription | string
ProtocolSupported | uint16
RequestedState | uint16
Status | string
StatusInfo | uint16
SystemCreationClassName | string
SystemName | string
TimeOfLastReset | datetime
TimeOfLastStateChange | datetime
TotalPowerOnHours | uint64
TransitioningToState | uint16
AdditionalAvailability | uint16[]
AvailableRequestedStates | uint16[]
IdentifyingDescriptions | string[]
OperationalStatus | uint16[]
OtherIdentifyingInfo | string[]
PowerManagementCapabilities | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
EnableDevice | uint32
OnlineDevice | uint32
QuiesceDevice | uint32
RequestStateChange | uint32
Reset | uint32
RestoreProperties | uint32
SaveProperties | uint32
SetPowerState | uint32