# Class CIM_PowerSource
extends CIM_LogicalDevice

This class is a representation of logical properties of a generic power source. Any logical device that has an aspect of producing power and thus effectively being a power source may be represented by this class or the subclass of this class.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_PowerSource

## Direct Known Subclasses

CIM_PowerSupply

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class is a representation of logical properties of a generic power source. Any logical device that has an aspect of producing power and thus effectively being a power source may be represented by this class or the subclass of this class.
UMLPackagePath | string | CIM::Device::CoolingAndPower
Version | string | 2.27.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
IsACOutput | boolean |
Description | string | A value of true shall indicate the output from the PowerSource is alternating current (AC). A value of false shall indicate the output from the PowerSource is direct current (DC).
OutputPowerUnits | string |
Description | string | Indicates the programatic units for the MaxOutputPower property.
ISPunit | boolean | true
ModelCorrespondence | string | CIM_PowerSource.RatedMaxOutputPower
RatedMaxOutputPower | uint32 |
Description | string | Indicates the maximum amount of power that may be drawn within the rating of the PowerSource. The units of the value shall be described by the OutputPowerUnits property. A value of zero shall indicate 'unknown'.
ModelCorrespondence | string | CIM_PowerSource.OutputPowerUnits

### Inherited Properties

Name | Data Type
--- | ---
AllocationState | string
Availability | uint16
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
DeviceID | string
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
ErrorCleared | boolean
ErrorDescription | string
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LastErrorCode | uint32
LocationIndicator | uint16
MaxQuiesceTime | uint64
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PowerManagementSupported | boolean
PowerOnHours | uint64
PrimaryStatus | uint16
RequestedState | uint16
Status | string
StatusInfo | uint16
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TotalPowerOnHours | uint64
TransitioningToState | uint16
AdditionalAvailability | uint16[]
AvailableRequestedStates | uint16[]
IdentifyingDescriptions | string[]
OperationalStatus | uint16[]
OtherIdentifyingInfo | string[]
PowerManagementCapabilities | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
EnableDevice | uint32
OnlineDevice | uint32
QuiesceDevice | uint32
RequestStateChange | uint32
Reset | uint32
RestoreProperties | uint32
SaveProperties | uint32
SetPowerState | uint32