# Class CIM_AlarmDevice
extends CIM_LogicalDevice

An AlarmDevice is a type of Device that emits audible or visible indications related to a problem situation.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_AlarmDevice

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | An AlarmDevice is a type of Device that emits audible or visible indications related to a problem situation.
UMLPackagePath | string | CIM::Device::Sensors
Version | string | 2.8.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AlarmState | uint16 |
Description | string | The current state of the alarm.
ValueMap | string | 0, 1, 2, 3
Values | string | Unknown, Off, Steady, Alternating
AudibleAlarm | boolean |
Description | string | Boolean indicating that the Alarm is audible.
AudioIndicatorIsDisabled | boolean |
Description | string | True indicates that the audio of an AlarmState indicator has been disabled (i.e. muted). A disabled state here does not imply that the AlarmState is off.
MotionAlarm | boolean |
Description | string | Boolean indicating that the Alarm causes motion of the Device.
MotionIndicatorIsDisabled | boolean |
Description | string | True indicates that the motion of an AlarmState indicator has been disabled (i.e. stopped). A disabled state here does not imply that the AlarmState is off.
Urgency | uint16 |
Description | string | Urgency is an enumerated value that indicates the relative frequency at which the Alarm flashes, vibrates and/or emits audible tones.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6
Values | string | Unknown, Other, Not Supported, Informational, Non-Critical, Critical, Unrecoverable
VisibleAlarm | boolean |
Description | string | Boolean indicating that the Alarm is visible.
VisualIndicatorIsDisabled | boolean |
Description | string | True indicates that the visual of an AlarmState indicator has been disabled (i.e. dimmed). A disabled state here does not imply that the AlarmState is off.

### Inherited Properties

Name | Data Type
--- | ---
AllocationState | string
Availability | uint16
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
DeviceID | string
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
ErrorCleared | boolean
ErrorDescription | string
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LastErrorCode | uint32
LocationIndicator | uint16
MaxQuiesceTime | uint64
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PowerManagementSupported | boolean
PowerOnHours | uint64
PrimaryStatus | uint16
RequestedState | uint16
Status | string
StatusInfo | uint16
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TotalPowerOnHours | uint64
TransitioningToState | uint16
AdditionalAvailability | uint16[]
AvailableRequestedStates | uint16[]
IdentifyingDescriptions | string[]
OperationalStatus | uint16[]
OtherIdentifyingInfo | string[]
PowerManagementCapabilities | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
EnableDevice | uint32
OnlineDevice | uint32
QuiesceDevice | uint32
RequestStateChange | uint32
Reset | uint32
RestoreProperties | uint32
SaveProperties | uint32
SetPowerState | uint32