# Class CIM_UninterruptiblePowerSupply
extends CIM_PowerSupply

Capabilities and management of an UninterruptiblePowerSupply. The properties of the UPS Device indicate when incoming power is trimmed or boosted, and the aggregated information of the batteries, generators, and so on that comprise the Device. These individual components (for example, multiple batteries) can also be independently modeled and associated with the UPS.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_PowerSource
|
+--CIM_PowerSupply
|
+--CIM_UninterruptiblePowerSupply

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Capabilities and management of an UninterruptiblePowerSupply. The properties of the UPS Device indicate when incoming power is trimmed or boosted, and the aggregated information of the batteries, generators, and so on that comprise the Device. These individual components (for example, multiple batteries) can also be independently modeled and associated with the UPS.
UMLPackagePath | string | CIM::Device::CoolingAndPower
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
EstimatedChargeRemaining | uint16 |
Description | string | An estimate of the percentage of full charge remaining for a UPS (that uses battery technology).
Gauge | boolean | true
MappingStrings | string | MIF.DMTF|UPS Battery|001.4
PUnit | string | percent
Units | string | Percent
EstimatedRunTime | uint32 |
Description | string | EstimatedRunTime is an estimate in minutes of the time that depletion of the battery, generator, or other device, will occur under the present load conditions if the utility power is off or is lost and remains off.
MappingStrings | string | MIF.DMTF|UPS Battery|001.3
PUnit | string | minute
Units | string | Minutes
Range1InputVoltageHigh | uint32 |
Description | string | If the voltage (in millivolts) rises above the value specified by Range1InputVoltageHigh, the UPS will compensate by trimming the voltage. A value of 0 indicates that the voltage at which trimming occurs is 'unknown'.
MappingStrings | string | MIF.DMTF|Power Supply|004.8
Override | string | Range1InputVoltageHigh
PUnit | string | volt * 10^-3
Units | string | MilliVolts
Range1InputVoltageLow | uint32 |
Description | string | If the voltage (in millivolts) drops below the value specified by Range1InputVoltageLow, the UPS will compensate by boosting the voltage using its power sources. A value of 0 indicates that the voltage at which boosting occurs is 'unknown'.
MappingStrings | string | MIF.DMTF|Power Supply|004.7
Override | string | Range1InputVoltageLow
PUnit | string | volt * 10^-3
Units | string | MilliVolts
Range2InputVoltageHigh | uint32 |
Description | string | If the voltage (in millivolts) rises above the value specified by Range2InputVoltageHigh, the UPS will compensate by trimming the voltage. A value of 0 indicates that the voltage at which trimming occurs is 'unknown'.
MappingStrings | string | MIF.DMTF|Power Supply|004.12
Override | string | Range2InputVoltageHigh
PUnit | string | volt * 10^-3
Units | string | MilliVolts
Range2InputVoltageLow | uint32 |
Description | string | If the voltage (in millivolts) drops below the value specified by Range2InputVoltageLow, the UPS will compensate by boosting the voltage using its power sources. A value of 0 indicates that the voltage at which boosting occurs is 'unknown'.
MappingStrings | string | MIF.DMTF|Power Supply|004.11
Override | string | Range2InputVoltageLow
PUnit | string | volt * 10^-3
Units | string | MilliVolts
RemainingCapacityStatus | uint16 |
Description | string | The indication of the capacity that remains in the UPS batteries, generator, and so on. A value of "Normal" (2) indicates that the remaining estimated minutes of run-time are greater than the 'low power' state defined for the UPS (typically two minutes). A value of "Low" (3) indicates that the remaining estimated minutes of run-time are less than or equal to the defined 'low power' state of the device. A value of "Depleted" (4) indicates that the UPS will be unable to sustain the present load when and if the utility power is lost (including the possibility that the utility power is currently absent).
MappingStrings | string | MIF.DMTF|UPS Battery|001.1
ValueMap | string | 1, 2, 3, 4
Values | string | Unknown, Normal, Low, Depleted
TimeOnBackup | uint32 |
Description | string | TimeOnBackup indicates the elapsed time in seconds since the UPS last switched to battery power, generator, or so on or the time since the UPS was last restarted, whichever is less. 0 is returned if the UPS is 'on line'.
MappingStrings | string | MIF.DMTF|UPS Battery|001.2
PUnit | string | second
Units | string | Seconds

### Inherited Properties

Name | Data Type
--- | ---
ActiveInputVoltage | uint16
AllocationState | string
Availability | uint16
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
DeviceID | string
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
ErrorCleared | boolean
ErrorDescription | string
Generation | uint64
HealthState | uint16
InputPowerUnits | string
InstallDate | datetime
InstanceID | string
IsACInput | boolean
IsACOutput | boolean
IsSwitchingSupply | boolean
LastErrorCode | uint32
LocationIndicator | uint16
MaxQuiesceTime | uint64
Name | string
NumberOfPhasesUtilized | uint32
OperatingStatus | uint16
OtherEnabledState | string
OutputPowerUnits | string
PowerManagementSupported | boolean
PowerOnHours | uint64
PrimaryStatus | uint16
Range1InputFrequencyHigh | uint32
Range1InputFrequencyLow | uint32
Range1MaxInputPower | uint32
Range1MaxOutputPower | uint32
Range2InputFrequencyHigh | uint32
Range2InputFrequencyLow | uint32
Range2MaxInputPower | uint32
Range2MaxOutputPower | uint32
RatedMaxOutputPower | uint32
RequestedState | uint16
Status | string
StatusInfo | uint16
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TotalOutputPower | uint32
TotalPowerOnHours | uint64
TransitioningToState | uint16
TypeOfRangeSwitching | uint16
AdditionalAvailability | uint16[]
AvailableRequestedStates | uint16[]
IdentifyingDescriptions | string[]
NominalPhaseWiring | uint32[]
OperationalStatus | uint16[]
OtherIdentifyingInfo | string[]
PowerManagementCapabilities | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
EnableDevice | uint32
OnlineDevice | uint32
QuiesceDevice | uint32
RequestStateChange | uint32
Reset | uint32
RestoreProperties | uint32
SaveProperties | uint32
SetPowerState | uint32