# Class CIM_PCVideoController
extends CIM_VideoController

Note: The use of the CIM_PCVideoController class has been deprecated in lieu of CIM_DisplayController. Deprecated description: Capabilities and management of a PCVideoController, a subtype of VideoController.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_Controller
|
+--CIM_VideoController
|
+--CIM_PCVideoController

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Deprecated | string | CIM_DisplayController
Description | string | Note: The use of the CIM_PCVideoController class has been deprecated in lieu of CIM_DisplayController. Deprecated description: Capabilities and management of a PCVideoController, a subtype of VideoController.
UMLPackagePath | string | CIM::Device::Controller
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
NumberOfColorPlanes | uint16 |
Deprecated | string | No value
Description | string | Current number of color planes. If this value is not applicable for the current video configuration, enter 0.
VideoArchitecture | uint16 |
Deprecated | string | No value
Description | string | The video architecture. For example, VGA (value=5) or PC-98 (160) can be specified.
MappingStrings | string | MIF.DMTF|Video|004.2
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 160
Values | string | Other, Unknown, CGA, EGA, VGA, SVGA, MDA, HGC, MCGA, 8514A, XGA, Linear Frame Buffer, PC-98
VideoMode | uint16 |
Deprecated | string | No value
Description | string | Current video mode.
MappingStrings | string | MIF.DMTF|Video|004.3

### Inherited Properties

Name | Data Type
--- | ---
AllocationState | string
Availability | uint16
Caption | string
CommunicationStatus | uint16
CreationClassName | string
CurrentBitsPerPixel | uint32
CurrentHorizontalResolution | uint32
CurrentNumberOfColors | uint64
CurrentNumberOfColumns | uint32
CurrentNumberOfRows | uint32
CurrentRefreshRate | uint32
CurrentScanMode | uint16
CurrentVerticalResolution | uint32
Description | string
DetailedStatus | uint16
DeviceID | string
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
ErrorCleared | boolean
ErrorDescription | string
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LastErrorCode | uint32
LocationIndicator | uint16
MaxMemorySupported | uint32
MaxNumberControlled | uint32
MaxQuiesceTime | uint64
MaxRefreshRate | uint32
MinRefreshRate | uint32
Name | string
NumberOfVideoPages | uint32
OperatingStatus | uint16
OtherEnabledState | string
PowerManagementSupported | boolean
PowerOnHours | uint64
PrimaryStatus | uint16
ProtocolDescription | string
ProtocolSupported | uint16
RequestedState | uint16
Status | string
StatusInfo | uint16
SystemCreationClassName | string
SystemName | string
TimeOfLastReset | datetime
TimeOfLastStateChange | datetime
TotalPowerOnHours | uint64
TransitioningToState | uint16
VideoMemoryType | uint16
VideoProcessor | string
AcceleratorCapabilities | uint16[]
AdditionalAvailability | uint16[]
AvailableRequestedStates | uint16[]
CapabilityDescriptions | string[]
IdentifyingDescriptions | string[]
OperationalStatus | uint16[]
OtherIdentifyingInfo | string[]
PowerManagementCapabilities | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
EnableDevice | uint32
OnlineDevice | uint32
QuiesceDevice | uint32
RequestStateChange | uint32
Reset | uint32
RestoreProperties | uint32
SaveProperties | uint32
SetPowerState | uint32