# Class CIM_DisplayController
extends CIM_Controller

Capabilities and management of the DisplayController.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_Controller
|
+--CIM_DisplayController

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Capabilities and management of the DisplayController.
UMLPackagePath | string | CIM::Device::Controller
Version | string | 2.31.1

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
Description | string |
Description | string | The Description property provides a textual description of the object.
MappingStrings | string | MIF.DMTF|Video|004.18
Override | string | Description
MaxMemorySupported | uint32 |
Description | string | Maximum amount of memory supported in bytes.
PUnit | string | byte
Units | string | Bytes
NumberOfVideoPages | uint32 |
Description | string | Number of video pages supported given the current resolutions and available memory.
OtherVideoArchitecture | string |
Description | string | A string describing the video architecture type when the instance's VideoArchitecture property is 1 ("Other").
ModelCorrespondence | string | CIM_DisplayController.VideoArchitecture
OtherVideoMemoryType | string |
Description | string | A string describing the video memory type when the instance's VideoMemoryType property is 1 ("Other").
ModelCorrespondence | string | CIM_DisplayController.VideoMemoryType
VideoArchitecture | uint16 |
Description | string | An integer enumeration indicating the display controllers video architecture used to generate the video signal. Usually, a dedicated video processor generates the video signal in accordance with the specified architecture.It is an indicator of the maximum resolution capability of the display controller.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 160, .., 0x8000..
Values | string | Unknown, Other, CGA, EGA, VGA, SVGA, MDA, HGC, MCGA, 8514A, XGA, Linear Frame Buffer, PC-98, DMTF Reserved, Vendor Reserved
VideoMemoryType | uint16 |
Description | string | An integer enumeration indicating the type of video memory.
MappingStrings | string | MIF.DMTF|Video|004.6
ModelCorrespondence | string | CIM_DisplayController.OtherVideoMemoryType
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12
Values | string | Unknown, Other, VRAM, DRAM, SRAM, WRAM, EDO RAM, Burst Synchronous DRAM, Pipelined Burst SRAM, CDRAM, 3DRAM, SDRAM, SGRAM
VideoProcessor | string |
Description | string | A free-form string describing the video processor/Controller.
AcceleratorCapabilities | uint16[] |
ArrayType | string | Indexed
Description | string | An array of integers indicating the graphics and 3D capabilities of the DisplayController.
ModelCorrespondence | string | CIM_DisplayController.CapabilityDescriptions
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8
Values | string | Unknown, Other, Graphics Accelerator, 3D Accelerator, PCI Fast Write, MultiMonitor Support, PCI Mastering, Second Monochrome Adapter Support, Large Memory Address Support
CapabilityDescriptions | string[] |
ArrayType | string | Indexed
Description | string | An array of free-form strings providing more detailed explanations for any of the video Accelerator features indicated in the Capabilities array. Note, each entry of this array is related to the entry in the Capabilities array that is located at the same index.
ModelCorrespondence | string | CIM_DisplayController.AcceleratorCapabilities

### Inherited Properties

Name | Data Type
--- | ---
AllocationState | string
Availability | uint16
Caption | string
CommunicationStatus | uint16
CreationClassName | string
DetailedStatus | uint16
DeviceID | string
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
ErrorCleared | boolean
ErrorDescription | string
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LastErrorCode | uint32
LocationIndicator | uint16
MaxNumberControlled | uint32
MaxQuiesceTime | uint64
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PowerManagementSupported | boolean
PowerOnHours | uint64
PrimaryStatus | uint16
ProtocolDescription | string
ProtocolSupported | uint16
RequestedState | uint16
Status | string
StatusInfo | uint16
SystemCreationClassName | string
SystemName | string
TimeOfLastReset | datetime
TimeOfLastStateChange | datetime
TotalPowerOnHours | uint64
TransitioningToState | uint16
AdditionalAvailability | uint16[]
AvailableRequestedStates | uint16[]
IdentifyingDescriptions | string[]
OperationalStatus | uint16[]
OtherIdentifyingInfo | string[]
PowerManagementCapabilities | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
EnableDevice | uint32
OnlineDevice | uint32
QuiesceDevice | uint32
RequestStateChange | uint32
Reset | uint32
RestoreProperties | uint32
SaveProperties | uint32
SetPowerState | uint32