# Class CIM_PrintInterpreter
extends CIM_PrinterElement

This class represents the PrintInterpreter component of a Printer (print device). It contains properties that describe the PrintInterpreter, including language type, language level, maximum resolution, default input character set, and status. Note: A PrintInterpreter shall be associated with exactly one Printer via an instance of the PrinterComponent class. A PrintInterpreter may be associated with a PrintChannel (for Job Control Language or Page Description Language defaults) via an instance of AssociatedPrintInterpreter. See: Model in section 2 of Printer MIB (RFC 3805).

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_PrinterElement
|
+--CIM_PrintInterpreter

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class represents the PrintInterpreter component of a Printer (print device). It contains properties that describe the PrintInterpreter, including language type, language level, maximum resolution, default input character set, and status. Note: A PrintInterpreter shall be associated with exactly one Printer via an instance of the PrinterComponent class. A PrintInterpreter may be associated with a PrintChannel (for Job Control Language or Page Description Language defaults) via an instance of AssociatedPrintInterpreter. See: Model in section 2 of Printer MIB (RFC 3805).
MappingStrings | string | MIB.IETF|Printer-MIB.prtInterpreterEntry
UMLPackagePath | string | CIM::Device::Printing
Version | string | 2.31.1

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AddressabilityBasis | uint16 |
Description | string | The basis for the limit properties FeedAddressability and XFeedAddressability, that specifies whether meaningful values are available. 1 (Other) means the PrintInterpreter places no restrictions on addressability and FeedAddressability and XFeedAddressability shall be null. 2 (Unknown) means the PrintInterpreter does not have meaningful values and FeedAddressability and XFeedAddressability shall be null. 3 (Actual) means the PrintInterpreter does have meaningful values and FeedAddressability and XFeedAddressability shall be present.
MappingStrings | string | MIB.IETF|Printer-MIB.prtInterpreterFeedAddressability, MIB.IETF|Printer-MIB.prtInterpreterXFeedAddressability
ModelCorrespondence | string | CIM_PrintInterpreter.FeedAddressability, CIM_PrintInterpreter.XFeedAddressability
ValueMap | string | 1, 2, 3, ..
Values | string | Other, Unknown, Actual, DMTF Reserved
AvailabilityStatus | uint32 |
Description | string | This property contains detailed availability information for this PrintInterpreter, as follows: 1 (Other) means other detailed availability information is present in the OtherAvailabilityStatus property. 2 (Unknown) means detailed availability information for this PrintInterpreter is unknown. 3 (AvailableIdle) means this PrintInterpreter is available and idle, i.e., not currently in use. 4 (AvailableStandy) means this PrintInterpreter is available but on standby, e.g., in a power saving mode. 5 (AvailableActive) means this PrintInterpreter is available and active, i.e., currently in use. 6 (AvailableBusy) means this PrintInterpreter is available but busy, i.e., not immediately available for its primary function. 7 (UnavailableOnRequest) means this PrintInterpreter is not available and is on request, i.e., needs human intervention. 8 (UnavailableBroken) means this PrintInterpreter is not available and is broken, e.g., needs repair/replacement.
MappingStrings | string | MIB.IETF|Printer-MIB.PrtSubUnitStatusTC
ModelCorrespondence | string | CIM_ManagedSystemElement.OperatingStatus, CIM_PrintInterpreter.OtherAvailabilityStatus
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, 8, ..
Values | string | Other, Unknown, AvailableIdle, AvailableStandby, AvailableActive, AvailableBusy, UnavailableOnRequest, UnavailableBroken, DMTF Reserved
CriticalAlertsPresent | boolean |
Description | string | If true, there are currently critical alerts on this PrintInterpreter.
MappingStrings | string | MIB.IETF|Printer-MIB.PrtSubUnitStatusTC
ModelCorrespondence | string | CIM_ManagedSystemElement.DetailedStatus
DefaultCharSetIn | string |
Description | string | The default character set for input octets encountered by the PrintInterpreter outside of a context in which a Page Description Language (PDL) has established the interpretation of the octets, e.g., when the value of the LangType property is equal to 30 (LangSimpleText).
MappingStrings | string | MIB.IETF|Printer-MIB.prtInterpreterDefaultCharSetIn, MIB.IETF|Printer-MIB.prtLocalizationCharacterSet, MIB.IETF|IANA-CHARSET-MIB.IANACharset
MaxLen | uint32 | 63
ModelCorrespondence | string | CIM_PrintInterpreter.LangType
FeedAddressability | uint32 |
Description | string | The maximum addressability (often called resolution) of this PrintInterpreter in dots per inch in the feed direction, i.e., long-edge in portrait feed mode.
MappingStrings | string | MIB.IETF|Printer-MIB.prtInterpreterFeedAddressability
MaxValue | sint64 | 2147483647
MinValue | sint64 | 0
ModelCorrespondence | string | CIM_PrintInterpreter.AddressabilityBasis, CIM_PrintInterpreter.XFeedAddressability
Punit | string | dot / inch
LangLevel | string |
Description | string | The level of the language which this PrintInterpreter is interpreting or emulating. For example, this property might contain: (a) a value of '5e' for a PrinterInterpreter which is emulating level 5e of the PCL; (b) a value of '2' for a PrinterInterpreter which is emulating level 2 of the PostScript language; or (c) a value of '2' for a PrinterInterpreter which is emulating level 2 of the HPGL language.
MappingStrings | string | MIB.IETF|Printer-MIB.prtInterpreterLangLevel
MaxLen | uint32 | 31
ModelCorrespondence | string | CIM_PrintInterpreter.LangType, CIM_PrintInterpreter.OtherLangTypeDescription
LangType | uint32 |
Description | string | The language type of a Page Description Language (PDL) or Job Control Language (JCL) which this PrintInterpreter can interpret or emulate.
MappingStrings | string | MIB.IETF|Printer-MIB.prtInterpreterLangFamily, MIB.IETF|IANA-PRINTER-MIB.PrtInterpreterLangFamilyTC
ModelCorrespondence | string | CIM_PrintInterpreter.OtherLangTypeDescription, CIM_PrintInterpreter.LangLevel
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23, 24, 25, 26, 27, 28, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 43, 44, 45, 46, 47, 48, 49, 50, 51, 52, 53, 54, 55, 56, 57, 58, 59, 60, 61, 62, 63, 64, 65, 66, 67, .., 32768..65535
Values | string | Other, Unknown, LangPCL, LangHPGL, LangPJL, LangPS, LangIPDS, LangPPDS, LangEscapeP, LangEpson, LangDDIF, LangInterpress, LangISO6429, LangLineData, LangMODCA, LangREGIS, LangSCS, LangSPDL, LangTEK4014, LangPDS, LangIGP, LangCodeV, LangDSCDSE, LangWPS, LangLN03, LangCCITT, LangQUIC, LangCPAP, LangDecPPL, LangSimpleText, LangNPAP, LangDOC, LangimPress, LangPinwriter, LangNPDL, LangNEC201PL, LangAutomatic, LangPages, LangLIPS, LangTIFF, LangDiagnostic, LangPSPrinter, LangCaPSL, LangEXCL, LangLCDS, LangXES, LangPCLXL, LangART, LangTIPSI, LangPrescribe, LangLinePrinter, LangIDP, LangXJCL, LangPDF, LangRPDL, LangIntermecIPL, LangUBIFingerprint, LangUBIDirectProtocol, LangFujitsu, LangCGM, LangJPEG, LangCALS1, LangCALS2, LangNIRS, LangC4, LangXPS, LangOpenXPS, DMTF Reserved, Vendor Reserved
LocalizedDescription | string |
Description | string | A free-form text description of this PrintInterpreter in the localization specified by CIM_Printer.CurrentNaturalLanguage.
MappingStrings | string | MIB.IETF|Printer-MIB.prtInterpreterDescription, MIB.IETF|Printer-MIB.PrtLocalizedDescriptionStringTC
MaxLen | uint32 | 255
NonCriticalAlertsPresent | boolean |
Description | string | If true, there are currently non-critical alerts on this PrintInterpreter.
MappingStrings | string | MIB.IETF|Printer-MIB.PrtSubUnitStatusTC
ModelCorrespondence | string | CIM_ManagedSystemElement.DetailedStatus
OtherAvailabilityStatus | string |
Description | string | A free-form string that describes the detailed availability of this PrintInterpreter when the value of the AvailabilityStatus property is equal to 1 (Other).
MaxLen | uint32 | 255
ModelCorrespondence | string | CIM_PrintInterpreter.AvailabilityStatus
OtherLangTypeDescription | string |
Description | string | A free-form string that describes the type of language when the value of the LangType property is equal to 1 (Other).
MaxLen | uint32 | 255
ModelCorrespondence | string | CIM_PrintInterpreter.LangType, CIM_PrintInterpreter.LangLevel
XFeedAddressability | uint32 |
Description | string | The maximum addressability (often called resolution) of this PrintInterpreter in dots per inch in the cross-feed direction, i.e., short-edge in portrait feed mode.
MappingStrings | string | MIB.IETF|Printer-MIB.prtInterpreterXFeedAddressability
MaxValue | sint64 | 2147483647
MinValue | sint64 | 0
ModelCorrespondence | string | CIM_PrintInterpreter.AddressabilityBasis, CIM_PrintInterpreter.FeedAddressability
Punit | string | dot / inch

### Inherited Properties

Name | Data Type
--- | ---
Caption | string
CommunicationStatus | uint16
Description | string
DetailedStatus | uint16
ElementName | string
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
Name | string
OperatingStatus | uint16
PrimaryStatus | uint16
SNMPRowId | uint32
Status | string
OperationalStatus | uint16[]
StatusDescriptions | string[]

## Class Methods