# Class CIM_FCPort
extends CIM_NetworkPort

Capabilities and management of a Fibre Channel Port Device.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_LogicalPort
|
+--CIM_NetworkPort
|
+--CIM_FCPort

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Capabilities and management of a Fibre Channel Port Device.
UMLPackagePath | string | CIM::Device::FC
Version | string | 2.45.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
DetailedPortState | uint16 |
Description | string | Additional port state/status information for the FCPort beyond that provided in OperationalStatus and EnabledState. The following detailed port states may occur when OperationStatus is set to OK: Transceiver Validation(2) indicates that the transceiver is being validated. Locking To Reference Signal(3) indicates that the port is locking to the reference signal. Sync (4) indicates the port is receiving light and is synchronized with the other port. The following detailed port states may occur when OperationStatus is set to Error: Invalid Transceiver (5) indicates the port has detected an invalid transceiver. No Light (6) indicates transciever is not receiving light. No Sync (7) indicates that port is receiving light but cannot synchronize. Laser Fault (8) indicates the transceiver is reporting the laser is not working or the transceiver is not reporting data for the laser, or software detected the error by polling the transceiver and shut the port down Port Fault (9) indicates the port encountered errors beyond the transceiver including excessive low level link initializations. Diagnostic Fault (10) indicates that diagnoistic tests running various traffic types.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, .., 0x8000..
Values | string | Unknown, Other, Transceiver Validation, Locking To Reference Signal, Sync, Invalid Transceiver, No Light, No Sync, Laser Fault, Port Fault, Diagnostic Fault, Vendor Reserved, DMTF Reserved
DomainPortNumber | uint16 |
Description | string | The port number used for domain id and physical port zone members.
LogicalModulePortNumber | uint16 |
Description | string | The port number labeled for an administrative purposes relative to the logical module.
PortAvailability | uint16 | 2
Description | string | The availability of the port for a client to determine whether the port can be made operational. The values: Available (2) indicates that the port can be made operational, Not Installed (3) indicates some aspect of the port has not been installed preventing it from being operational but is discoverable through instrumentation, No Transceiver (4) indicates that the transceiver is not installed to allow the port to become operational, Not Licensed (5) indicates that the port cannot be made operational due to a license not existing for the port.
ValueMap | string | 0, 2, 3, 4, 5, ..
Values | string | Unknown, Available, Not Installed, No Transceiver, Not Licensed, DMTF Reserved
PortNumber | uint16 |
Description | string | The labeled port number for administrative purposes. This is typically what is exposed through the devices element manager or CLI.
Override | string | PortNumber
PortType | uint16 |
Description | string | The specific mode currently enabled for the Port. If the port is logged in, this will be the negotiated port type, otherwise the configured port type will be reported. The values: "N" = Node Port, "NL" = Node Port supporting FC arbitrated loop, "NX" = Port may negotiate to become either a node port (N) or a node port supporting FC arbitrated loop (NL), "E" = Expansion Port connecting fabric elements (for example, FC switches), "F" = Fabric (element) Port, "FL" = Fabric (element) Port supporting FC arbitrated loop, "FX" = Port may negotiate to become a fabric port (F), or a fabric port supporting FC arbitrated loop (FL). "B" = Bridge port, and "G" = Port may negotiate to become either an expansion port (E), or a fabric port (F), "GL" = Port may negotiate to become an expansion port (E), a fabric port (F), or a fabric port supporting FC arbitrated loop (FL). PortTypes are defined in the ANSI X3 standards. When set to 1 ("Other"), the related property OtherPortType contains a string description of the type of port.
ModelCorrespondence | string | CIM_NetworkPort.OtherNetworkPortType
Override | string | PortType
ValueMap | string | 0, 1, 10, 11, 12, 13, 14, 15, 16, 17, 18, 16000..65535
Values | string | Unknown, Other, N, NL, F/NL, Nx, E, F, FL, B, G, Vendor Reserved
ActiveCOS | uint16[] |
Description | string | An array of integers that indicates the Classes of Service that are active. The Active COS is indicated in ActiveCOS.
ModelCorrespondence | string | CIM_FCPort.SupportedCOS
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7
Values | string | Unknown, 1, 2, 3, 4, 5, 6, F
ActiveFC4Types | uint16[] |
Description | string | An array of integers that indicates the Fibre Channel FC-4 protocols currently running. A list of all supported protocols is indicated in the SupportedFC4Types property.
ModelCorrespondence | string | CIM_FCPort.SupportedFC4Types
ValueMap | string | 0, 1, 4, 5, 8, 9, 17, 18, 19, 21, 22, 23, 25, 26, 27, 28, 32, 34, 36, 64, 80, 81, 82, 88, 96, 255..
Values | string | Unknown, Other, ISO/IEC 8802 - 2 LLC, IP over FC, SCSI - FCP, SCSI - GPP, IPI - 3 Master, IPI - 3 Slave, IPI - 3 Peer, CP IPI - 3 Master, CP IPI - 3 Slave, CP IPI - 3 Peer, SBCCS Channel, SBCCS Control Unit, FC-SB-2 Channel, FC-SB-2 Control Unit, Fibre Channel Services (FC-GS, FC-GS-2, FC-GS-3), FC-SW, FC - SNMP, HIPPI - FP, BBL Control, BBL FDDI Encapsulated LAN PDU, BBL 802.3 Encapsulated LAN PDU, FC - VI, FC - AV, Vendor Unique
PortDiscriminator | uint16[] |
Description | string | An enumeration used to discriminate the context in which this FCPort is instantiated: Not Applicable (2) indicates that this FCPort was not instantiated in any special context. VF (3) indicates this FCPort was instantiated in the context of Virtual Fabrics (VF). FCIP (4) indicates that this FCport was instantiated in the context of FC over IP (FCIP). IFR (5) indicates that this FCPort was instantiated in the context of Inter-Fabric Routing (IFR). IFR (Virtual) (6) indicates that this FCPort was instantiated in the context of Inter-Fabric Routing (IFR) and has no physical representation. NPIV (7) indicates that this FCPort was instantiated in the context of N Port Virtualization (NPIV). Internal (8) indicates that this FCPort is not externally visible and is represented physically internally in the hardware (unlike VF). Chassis (9) indicates that this FCPort is externally visible but is not supported by a traditional fibre channel connector (for example a chassis to chassis connection). FCoE (10) indicates that this FCPort is instantiated for Fibre Channel over Ethernet (FCoE). FC (Native) (11) indicates that this FCPort represents a native FCPort. HBA (12) indicates that this FCPort is instantiated in a Host Bus Adapter (HBA) context. Storage (13) indicates that this FCPort in instantiated in a storage (e.g., disk array) context.
ValueMap | string | 0, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, ..
Values | string | Unknown, Not Applicable, VF, FCIP, IFR, IFR (Virtual), NPIV, Internal, Chassis, FCoE, FC (Native), HBA, Storage, DMTF Reserved
SupportedCOS | uint16[] |
Description | string | An array of integers that indicates the Fibre Channel Classes of Service that are supported. The active COS are indicated in ActiveCOS.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7
Values | string | Unknown, 1, 2, 3, 4, 5, 6, F
SupportedFC4Types | uint16[] |
Description | string | An array of integers that indicates the Fibre Channel FC-4 protocols supported. The protocols that are active and running are indicated in the ActiveFC4Types property.
ValueMap | string | 0, 1, 4, 5, 8, 9, 17, 18, 19, 21, 22, 23, 25, 26, 27, 28, 32, 34, 36, 64, 80, 81, 82, 88, 96, 255..
Values | string | Unknown, Other, ISO/IEC 8802 - 2 LLC, IP over FC, SCSI - FCP, SCSI - GPP, IPI - 3 Master, IPI - 3 Slave, IPI - 3 Peer, CP IPI - 3 Master, CP IPI - 3 Slave, CP IPI - 3 Peer, SBCCS Channel, SBCCS Control Unit, FC-SB-2 Channel, FC-SB-2 Control Unit, Fibre Channel Services (FC-GS, FC-GS-2, FC-GS-3), FC-SW, FC - SNMP, HIPPI - FP, BBL Control, BBL FDDI Encapsulated LAN PDU, BBL 802.3 Encapsulated LAN PDU, FC - VI, FC - AV, Vendor Unique

### Inherited Properties

Name | Data Type
--- | ---
ActiveMaximumTransmissionUnit | uint64
AllocationState | string
AutoSense | boolean
Availability | uint16
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
DeviceID | string
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
ErrorCleared | boolean
ErrorDescription | string
FullDuplex | boolean
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LastErrorCode | uint32
LinkTechnology | uint16
LocationIndicator | uint16
MaxQuiesceTime | uint64
MaxSpeed | uint64
Name | string
OperatingStatus | uint16
OtherEnabledState | string
OtherLinkTechnology | string
OtherNetworkPortType | string
OtherPortType | string
PermanentAddress | string
PowerManagementSupported | boolean
PowerOnHours | uint64
PrimaryStatus | uint16
RequestedSpeed | uint64
RequestedState | uint16
Speed | uint64
Status | string
StatusInfo | uint16
SupportedMaximumTransmissionUnit | uint64
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TotalPowerOnHours | uint64
TransitioningToState | uint16
UsageRestriction | uint16
AdditionalAvailability | uint16[]
AvailableRequestedStates | uint16[]
IdentifyingDescriptions | string[]
NetworkAddresses | string[]
OperationalStatus | uint16[]
OtherIdentifyingInfo | string[]
PowerManagementCapabilities | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
EnableDevice | uint32
OnlineDevice | uint32
QuiesceDevice | uint32
RequestStateChange | uint32
Reset | uint32
RestoreProperties | uint32
SaveProperties | uint32
SetPowerState | uint32