# Class CIM_FCActiveConnection
extends CIM_ActiveConnection

This association specializes ActiveConnection to represent the connections between two Fibre Channel ProtocolEndpoints. The ActiveConnection can be an ISL, a Host to Switch Link, a Switch to Device Link, or a connection created

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_Dependency
|
+--CIM_SAPSAPDependency
|
+--CIM_ActiveConnection
|
+--CIM_FCActiveConnection

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Association | boolean | true
Description | string | This association specializes ActiveConnection to represent the connections between two Fibre Channel ProtocolEndpoints. The ActiveConnection can be an ISL, a Host to Switch Link, a Switch to Device Link, or a connection created
UMLPackagePath | string | CIM::Device::FC
Version | string | 2.45.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
Discriminator | uint16[] |
Description | string | An enumeration used to discriminate the context in which the ActiveConnectionis instantiated: Not Applicable(2) indicates that this ActiveConnection is not instantiated in any special context, VF(3) indicates that this ActiveConnection is instantiated in the context of Virtual Fabrics, NPIV(7) indicates that this ActiveConnection is instantiated in the context of N Port Virtualization (NPIV), Chassis(9) icdicates that this ActiveConnection is instantiated as part of a chassis to chassis connection, FCoE(10) indicates that this ActiveConnection is instatiated in the context of Fibre Channel over Ethernet (FCoE).
ValueMap | string | 0, 2, 3, 5, 7, 9, 10, ..
Values | string | Unknown, Not Applicable, VF, IFR, NPIV, Chassis, FCoE, DMTF Reserved

### Association References

Name | Reference Class
--- | ---

### Propagated Association References

Name | Reference Class
--- | ---

### Inherited Properties

Name | Data Type
--- | ---
IsUnidirectional | boolean
OtherTrafficDescription | string
TrafficType | uint16

## Class Methods