# Class CIM_SCSIProtocolEndpoint
extends CIM_ProtocolEndpoint

A SCSIProtocolEndpoint represents the protocol (command) aspects of a logical SCSI port, independent of the connection/transport. SCSIProtocolEndpoint is either directly or indirectly associated to one or more instances of LogicalPort (via DeviceSAPImplementation) depending on the underlying transport. Indirect associations aggregate one or more LogicalPorts using intermediate ProtocolEndpoints (iSCSI, etc). SCSIProtocolEndpoint is also associated to a SCSIProtocolController, representing the SCSI device.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_ServiceAccessPoint
|
+--CIM_ProtocolEndpoint
|
+--CIM_SCSIProtocolEndpoint

## Direct Known Subclasses

CIM_iSCSIProtocolEndpoint

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | A SCSIProtocolEndpoint represents the protocol (command) aspects of a logical SCSI port, independent of the connection/transport. SCSIProtocolEndpoint is either directly or indirectly associated to one or more instances of LogicalPort (via DeviceSAPImplementation) depending on the underlying transport. Indirect associations aggregate one or more LogicalPorts using intermediate ProtocolEndpoints (iSCSI, etc). SCSIProtocolEndpoint is also associated to a SCSIProtocolController, representing the SCSI device.
UMLPackagePath | string | CIM::Network::ProtocolEndpoints
Version | string | 2.45.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
ConnectionType | uint16 |
Description | string | The supported connection type for this endpoint. The connection type may be needed before the port(s) are associated and also is used in some SCSI commands.
MappingStrings | string | SPC.INCITS-T10 | Protocol Identifier | Values
ModelCorrespondence | string | CIM_SCSIProtocolEndpoint.Name, CIM_SCSIProtocolEndpoint.OtherConnectionType
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, 8, 9
Values | string | Other, Fibre Channel, Parallel SCSI, SSA, IEEE 1394, RDMA, iSCSI, SAS, ADT
Name | string |
Description | string | The SCSI identifier for the target or initiator device, in the format appropriate for the ConnectionType. If a ConnectionType specific subclass is defined, the subclass may override Name to define the format. For other ConnectionTypes, the format (and content) should match that of PermamnentAddress of the corresponding LogicalPort.
Key | boolean | true
MappingStrings | string | SPC.INCITS-T10 |Protocol Specific Parameters | Name
MaxLen | uint32 | 256
ModelCorrespondence | string | CIM_SCSIProtocolEndpoint.ConnectionType, CIM_SCSIProtocolEndpoint.OtherConnectionType
Override | string | Name
OtherConnectionType | string |
Description | string | The connection type, if ConnectionType is "Other".
ModelCorrespondence | string | CIM_SCSIProtocolEndpoint.Name, CIM_SCSIProtocolEndpoint.ConnectionType
Role | uint16 |
Description | string | For iSCSI, each SCSIProtocolEndpoint MUST act as either a target or an initiator endpoint. Other transports allow a SCSI PE to act as both an initiator and target endpoint. This property indicates which role this ProtocolEndpoint implements.
ValueMap | string | 0, 2, 3, 4
Values | string | Unknown, Initiator, Target, Both Initiator and Target
TargetRelativePortNumber | uint32 |
Description | string | For ports on a target device, the port number, relative to the storage system. 0 is reserved by T10, 1 is port A, 2 is port B, etc. These numbers are used in SCSI commands that operate on target port groups.
MappingStrings | string | SPC.INCITS-T10 | RelativeTargetPort | IdentifierFormat
MinValue | sint64 | 1

### Inherited Properties

Name | Data Type
--- | ---
BroadcastResetSupported | boolean
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
NameFormat | string
OperatingStatus | uint16
OtherEnabledState | string
OtherTypeDescription | string
PrimaryStatus | uint16
ProtocolIFType | uint16
ProtocolType | uint16
RequestedState | uint16
Status | string
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TransitioningToState | uint16
AvailableRequestedStates | uint16[]
OperationalStatus | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
BroadcastReset | uint32
RequestStateChange | uint32