# Class CIM_AGPVideoController
extends CIM_VideoController

Capabilities and management of an AGPVideoController.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_Controller
|
+--CIM_VideoController
|
+--CIM_AGPVideoController

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Capabilities and management of an AGPVideoController.
UMLPackagePath | string | CIM::Device::Controller
Version | string | 2.54.1

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AddressingMode | uint16 |
Description | string | An integer enumeration indicating the addressing mode of the graphics Controller.
ValueMap | string | 0, 1, 2, 3
Values | string | Unknown, Other, Sideband, Pipeline
AGPSpecificationVersionConformance | string |
Description | string | A string containing the AGP specification version to which this graphics Controller conforms.
DataTransferRate | uint16 |
Description | string | An integer enumeration indicating the data transfer rate of the graphics Controller.
ValueMap | string | 0, 1, 2, 3, 4
Values | string | Unknown, Other, 1X, 2X, 4X
GraphicsApertureSize | uint32 |
Description | string | Size of the graphics aperture in KB.
PUnit | string | byte * 2^10
Units | string | KiloBytes
LocalBusWidth | uint32 |
Description | string | Width of the internal bus in the graphics Controller, in bits.
PUnit | string | bit
Units | string | Bits
MaximumAGPCommandQueuePath | uint32 |
Description | string | The maximum number of AGP Transaction requests that the master (AGP Graphics Controller) is allowed to enqueue into the target.
MaxNumberOfPipelinedAGPTransactions | uint32 |
Description | string | The number of AGP Transaction that the core logic (chipset) can accept into its transaction request queue from the Controller.
NonlocalVideoMemorySize | uint32 |
Description | string | Size of the non-local video memory in KB.
PUnit | string | byte * 2^10
Units | string | KiloBytes
UsageModel | uint16 |
Description | string | An integer enumeration indicating the usage model of the graphics Controller. Usage model indicates how the Controller does manipulations of graphics surfaces, textures, etc. in memory. DMA indicates that the graphics Controller brings structures from the system memory to its local memory to perform needed manipulations or renderings. Execute specifies that the graphics Controller can directly access a specified region in main memory (called the graphics aperture) using GART - Graphics Aperture Remapping Table. It then performs manipulations in that range as if that whole graphics aperture were part of its local memory. A value of "Both" DMA and Execute models may also be specified.
ValueMap | string | 0, 1, 2, 3, 4
Values | string | Unknown, Other, Execute, DMA, Both
Capabilities | uint16[] |
ArrayType | string | Indexed
Deprecated | string | CIM_VideoController.AcceleratorCapabilities
Description | string | This property has been incorporated into the inherited AcceleratorCapabilities property. Capabilities of the AGP Graphics Controller. For example, the Device may support multiple monitors, PCI Mastering and large memory addresses. In this case, the values 3, 4 and 6 would be written to the Capabilities array.
ModelCorrespondence | string | CIM_AGPVideoController.CapabilityDescriptions
ValueMap | string | 0, 1, 2, 3, 4, 5, 6
Values | string | Unknown, Other, PCI Fast Write, MultiMonitor Support, PCI Mastering, Second Monochrome Adapter Support, Large Memory Address Support

### Inherited Properties

Name | Data Type
--- | ---
AllocationState | string
Availability | uint16
Caption | string
CommunicationStatus | uint16
CreationClassName | string
CurrentBitsPerPixel | uint32
CurrentHorizontalResolution | uint32
CurrentNumberOfColors | uint64
CurrentNumberOfColumns | uint32
CurrentNumberOfRows | uint32
CurrentRefreshRate | uint32
CurrentScanMode | uint16
CurrentVerticalResolution | uint32
Description | string
DetailedStatus | uint16
DeviceID | string
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
ErrorCleared | boolean
ErrorDescription | string
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LastErrorCode | uint32
LocationIndicator | uint16
MaxMemorySupported | uint32
MaxNumberControlled | uint32
MaxQuiesceTime | uint64
MaxRefreshRate | uint32
MinRefreshRate | uint32
Name | string
NumberOfVideoPages | uint32
OperatingStatus | uint16
OtherEnabledState | string
PowerManagementSupported | boolean
PowerOnHours | uint64
PrimaryStatus | uint16
ProtocolDescription | string
ProtocolSupported | uint16
RequestedState | uint16
Status | string
StatusInfo | uint16
SystemCreationClassName | string
SystemName | string
TimeOfLastReset | datetime
TimeOfLastStateChange | datetime
TotalPowerOnHours | uint64
TransitioningToState | uint16
VideoMemoryType | uint16
VideoProcessor | string
AcceleratorCapabilities | uint16[]
AdditionalAvailability | uint16[]
AvailableRequestedStates | uint16[]
CapabilityDescriptions | string[]
IdentifyingDescriptions | string[]
OperationalStatus | uint16[]
OtherIdentifyingInfo | string[]
PowerManagementCapabilities | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
EnableDevice | uint32
OnlineDevice | uint32
QuiesceDevice | uint32
RequestStateChange | uint32
Reset | uint32
RestoreProperties | uint32
SaveProperties | uint32
SetPowerState | uint32