# Class CIM_LANEndpoint
extends CIM_ProtocolEndpoint

A communication endpoint which, when its associated interface device is connected to a LAN, may send and receive data frames. LANEndpoints include Ethernet, Token Ring and FDDI interfaces.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_ServiceAccessPoint
|
+--CIM_ProtocolEndpoint
|
+--CIM_LANEndpoint

## Direct Known Subclasses

CIM_WiFiEndpoint

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | A communication endpoint which, when its associated interface device is connected to a LAN, may send and receive data frames. LANEndpoints include Ethernet, Token Ring and FDDI interfaces.
UMLPackagePath | string | CIM::Network::ProtocolEndpoints
Version | string | 2.54.1

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
LANID | string |
Description | string | A label or identifier for the LAN Segment to which the Endpoint is connected. If the Endpoint is not currently active/connected or this information is not known, then LANID is NULL.
ModelCorrespondence | string | CIM_LANConnectivitySegment.LANID, CIM_LANSegment.LANID
LANType | uint16 |
Deprecated | string | CIM_ProtocolEndpoint.ProtocolType
Description | string | An indication of the kind of technology used on the LAN. This property is deprecated in lieu of ProtocolType, which is an enumeration inherited from ProtocolEndpoint and which includes the Values specified here.
ModelCorrespondence | string | CIM_LANConnectivitySegment.ConnectivityType, CIM_LANSegment.LANType
ValueMap | string | 0, 1, 2, 3, 4
Values | string | Unknown, Other, Ethernet, TokenRing, FDDI
MACAddress | string |
Description | string | The principal unicast address used in communication with the LANEndpoint. The MAC address is formatted as twelve hexadecimal digits (e.g., "010203040506"), with each pair representing one of the six octets of the MAC address in "canonical" bit order according to RFC 2469.
MaxLen | uint32 | 12
MaxDataSize | uint32 |
Description | string | The largest information field that may be sent or received by the LANEndpoint.
PUnit | string | bit
Units | string | Bits
OtherLANType | string |
Deprecated | string | CIM_ProtocolEndpoint.OtherTypeDescription
Description | string | A free-form string that describes the type of technology used on the LAN when the value of the LANType property is equal to 1 (i.e., "Other"). This property is deprecated since its purpose overlaps with OtherTypeDescription, which which is inherited from ProtocolEndpoint.
ModelCorrespondence | string | CIM_LANConnectivitySegment.OtherTypeDescription, CIM_LANEndpoint.LANType
AliasAddresses | string[] |
Description | string | Other unicast addresses that may be used to communicate with the LANEndpoint.
GroupAddresses | string[] |
Description | string | Multicast addresses to which the LANEndpoint listens.

### Inherited Properties

Name | Data Type
--- | ---
BroadcastResetSupported | boolean
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
Name | string
NameFormat | string
OperatingStatus | uint16
OtherEnabledState | string
OtherTypeDescription | string
PrimaryStatus | uint16
ProtocolIFType | uint16
ProtocolType | uint16
RequestedState | uint16
Status | string
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TransitioningToState | uint16
AvailableRequestedStates | uint16[]
OperationalStatus | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
BroadcastReset | uint32
RequestStateChange | uint32