# Class CIM_iSCSILoginStatistics
extends CIM_StatisticalData

Statistics for Logins and Logouts to or from an iSCSI Node. An instance of this class will be associated by ElementStatisticalData to an instance of SCSIProtocolController that represents the Node. The Node can be either an Initiator or Target and so the interpretation of the properties in this class varies accordingly.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_StatisticalData
|
+--CIM_iSCSILoginStatistics

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Statistics for Logins and Logouts to or from an iSCSI Node. An instance of this class will be associated by ElementStatisticalData to an instance of SCSIProtocolController that represents the Node. The Node can be either an Initiator or Target and so the interpretation of the properties in this class varies accordingly.
UMLPackagePath | string | CIM::Network::iSCSI
Version | string | 2.11.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AuthenticationLoginFailures | uint64 |
Counter | boolean | true
Description | string | If the node is an initiator this property is the number of times it has aborted a login because the target could not be authenticated. If the node is a target this property is the count of Login Response PDUs with status 0x0201, Authentication Failed, transmitted by this target.
MappingStrings | string | MIB.IETF|iSCSI-MIB.iscsiIntrLoginAuthenticateFails, MIB.IETF|iSCSI-MIB.iscsiTgtLoginAuthenticateFails
AuthorizationLoginFailures | uint64 |
Counter | boolean | true
Description | string | If the node is an initiator this property is the count of Login Response PDUs with status class 0x201, 'Authentication Failed', received by this initiator. If the node is a target the property is the count of Login Response PDUs with status 0x0202, 'Forbidden Target', transmitted by this target.
MappingStrings | string | MIB.IETF|iSCSI-MIB.iscsiIntrLoginAuthFailRsps, MIB.IETF|iSCSI-MIB.iscsiTgtLoginAuthorizeFails
LastLoginFailureRemoteAddress | uint32 |
Description | string | An Internet Network Address giving the host address of the remote node that failed the last login attempt.
MappingStrings | string | MIB.IETF|iSCSI-MIB.iscsiIntrLastTgtFailureAddr, MIB.IETF|iSCSI-MIB.iscsiTgtLastIntrFailureAddr
ModelCorrespondence | string | CIM_iSCSILoginStatistics.LastLoginFailureRemoteNodeName, CIM_iSCSILoginStatistics.LastLoginFailureRemoteAddressType
LastLoginFailureRemoteAddressType | uint16 |
Description | string | The type of Internet Network Address of the remote node that failed the last login attempt.
MappingStrings | string | MIB.IETF|iSCSI-MIB.iscsiIntrLastTgtFailureAddrType, MIB.IETF|iSCSI-MIB.iscsiTgtLastIntrFailureAddrType
ModelCorrespondence | string | CIM_iSCSILoginStatistics.LastLoginFailureRemoteNodeName, CIM_iSCSILoginStatistics.LastLoginFailureRemoteAddress
ValueMap | string | 1, 2
Values | string | IPv4, IPv6
LastLoginFailureRemoteNodeName | string |
Description | string | The iSCSI name of the remote node that failed the last login attempt.
MappingStrings | string | MIB.IETF|iSCSI-MIB.iscsiIntrLastTgtFailureName, MIB.IETF|iSCSI-MIB.iscsiTgtLastIntrFailureName
ModelCorrespondence | string | CIM_iSCSILoginStatistics.LastLoginFailureTime, CIM_iSCSILoginStatistics.LastLoginFailureType, CIM_iSCSILoginStatistics.LastLoginFailureRemoteAddressType, CIM_iSCSILoginStatistics.LastLoginFailureRemoteAddress
LastLoginFailureTime | datetime |
Description | string | The timestamp of the most recent failure of a login attempt from this node(initiator) or to this node(target). A value of zero indicates that no such failures have occurred since the last system boot.
MappingStrings | string | MIB.IETF|iSCSI-MIB.iscsiIntrLastFailureTime, MIB.IETF|iSCSI-MIB.iscsiTgtLastFailureTime
ModelCorrespondence | string | CIM_iSCSILoginStatistics.LastLoginFailureType, CIM_iSCSILoginStatistics.LastLoginFailureRemoteNodeName
LastLoginFailureType | uint16 |
Description | string | The type of the most recent failure of a login attempt from this node(initiator) or to this node(target).
MappingStrings | string | MIB.IETF|iSCSI-MIB.iscsiIntrLastFailureType, MIB.IETF|iSCSI-MIB.iscsiTgtLastFailureType
ModelCorrespondence | string | CIM_iSCSILoginStatistics.OtherLastLoginFailureType, CIM_iSCSILoginStatistics.LastLoginFailureTime, CIM_iSCSILoginStatistics.LastLoginFailureRemoteNodeName
ValueMap | string | 1, 2, 3, 4, 5
Values | string | Other, Negotiate, Authenticate, Authorize, Redirect
LoginFailures | uint64 |
Counter | boolean | true
Description | string | This property counts the number of times a login attempt from this node(initiator) or to this node(target) has failed.
MappingStrings | string | MIB.IETF|iSCSI-MIB.iscsiIntrLoginFailures, MIB.IETF|iSCSI-MIB.iscsiTgtLoginFailures
LoginRedirects | uint64 |
Counter | boolean | true
Description | string | The count of Login Response PDUs with status class 0x01, Redirection, received by this node(initiator) or transmitted by this node(target).
MappingStrings | string | MIB.IETF|iSCSI-MIB.iscsiIntrLoginRedirectRsps, MIB.IETF|iSCSI-MIB.iscsiTgtLoginRedirects
NegotiationLoginFailures | uint64 |
Counter | boolean | true
Description | string | If the node is an initiator this property is the number of times it has aborted a login because parameter negotiation with the target failed. If the node is a target the property is the number of times a it has effectively refused a login because the parameter negotiation failed. While this situation can occur, the exact mechanism is as yet undefined in the iSCSI Protocol Spec.
MappingStrings | string | MIB.IETF|iSCSI-MIB.iscsiIntrLoginNegotiateFails, MIB.IETF|iSCSI-MIB.iscsiTgtLoginNegotiateFails
NormalLogouts | uint64 |
Counter | boolean | true
Description | string | The count of Logout Command PDUs generated by this node (initiator) or received by this node(target), with reason code 0 (closes the session).
MappingStrings | string | MIB.IETF|iSCSI-MIB.iscsiIntrLogoutNormals, MIB.IETF|iSCSI-MIB.iscsiTgtLogoutNormals
OtherLastLoginFailureType | string |
Description | string | A string describing the type of the last login failure when LastLoginFailureType is equal to the value 1, "Other".
ModelCorrespondence | string | CIM_iSCSILoginStatistics.LastLoginFailureType
OtherLoginFailures | uint64 |
Counter | boolean | true
Description | string | The number of failure Login Response PDUs which were received by this node(initiator) or were transmitted by this node(target), and which were not counted by any other property in this class.
MappingStrings | string | MIB.IETF|iSCSI-MIB.iscsiIntrLoginOtherFailRsps, MIB.IETF|iSCSI-MIB.iscsiTgtLoginOtherFails
OtherLogouts | uint64 |
Counter | boolean | true
Description | string | The count of Logout Command PDUs generated by this node, (initiator) or received by this node(target), with any reason code other than 0.
MappingStrings | string | MIB.IETF|iSCSI-MIB.iscsiIntrLogoutOthers, MIB.IETF|iSCSI-MIB.iscsiTgtLogoutOthers
SuccessfulLogins | uint64 |
Counter | boolean | true
Description | string | The count of Login Response PDUs with status 0x0000, Accept Login, received by this node(initator), or transmitted by this node (target).
MappingStrings | string | MIB.IETF|iSCSI-MIB.iscsiIntrLoginAcceptRsps, MIB.IETF|iSCSI-MIB.iscsiTgtLoginAccepts

### Inherited Properties

Name | Data Type
--- | ---
Caption | string
Description | string
ElementName | string
Generation | uint64
InstanceID | string
RateIntervalEndTime | datetime
RateIntervalStartTime | datetime
SampleInterval | datetime
StartStatisticTime | datetime
StatisticTime | datetime

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
ResetSelectedStats | uint32