# Class CIM_ParallelController
extends CIM_Controller

Capabilities and management of the ParallelController.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_Controller
|
+--CIM_ParallelController

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Capabilities and management of the ParallelController.
UMLPackagePath | string | CIM::Device::Controller
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
DMASupport | boolean |
Description | string | Set to true if the ParallelController supports DMA.
MappingStrings | string | MIF.DMTF|Parallel Ports|003.7
Security | uint16 |
Description | string | An enumeration that indicates the operational security for the Controller. For example, information that the external interface of the Device is locked out (value=4) or "Boot Bypass" (value=6) can be described using this property.
MappingStrings | string | MIF.DMTF|Parallel Ports|003.10
ValueMap | string | 1, 2, 3, 4, 5, 6
Values | string | Other, Unknown, None, External Interface Locked Out, External Interface Enabled, Boot Bypass
Capabilities | uint16[] |
ArrayType | string | Indexed
Description | string | An integer enumeration that indicates the capabilities of the ParallelController.
MappingStrings | string | MIF.DMTF|Parallel Ports|003.8
ModelCorrespondence | string | CIM_ParallelController.CapabilityDescriptions
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8
Values | string | Unknown, Other, XT/AT Compatible, PS/2 Compatible, ECP, EPP, PC-98, PC-98-Hireso, PC-H98
CapabilityDescriptions | string[] |
ArrayType | string | Indexed
Description | string | An array of free-form strings that provides more detailed explanations for any of the ParallelController features that are indicated in the Capabilities array. Note, each entry of this array is related to the entry in the Capabilities array that is located at the same index.
ModelCorrespondence | string | CIM_ParallelController.Capabilities

### Inherited Properties

Name | Data Type
--- | ---
AllocationState | string
Availability | uint16
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
DeviceID | string
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
ErrorCleared | boolean
ErrorDescription | string
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LastErrorCode | uint32
LocationIndicator | uint16
MaxNumberControlled | uint32
MaxQuiesceTime | uint64
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PowerManagementSupported | boolean
PowerOnHours | uint64
PrimaryStatus | uint16
ProtocolDescription | string
ProtocolSupported | uint16
RequestedState | uint16
Status | string
StatusInfo | uint16
SystemCreationClassName | string
SystemName | string
TimeOfLastReset | datetime
TimeOfLastStateChange | datetime
TotalPowerOnHours | uint64
TransitioningToState | uint16
AdditionalAvailability | uint16[]
AvailableRequestedStates | uint16[]
IdentifyingDescriptions | string[]
OperationalStatus | uint16[]
OtherIdentifyingInfo | string[]
PowerManagementCapabilities | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
EnableDevice | uint32
OnlineDevice | uint32
QuiesceDevice | uint32
RequestStateChange | uint32
Reset | uint32
RestoreProperties | uint32
SaveProperties | uint32
SetPowerState | uint32