# Class CIM_RoutingProtocolDomain
extends CIM_AdminDomain

A Routing Protocol Domain is a collection of routers which coordinate their routing knowledge using a single [instance of a] routing protocol. This class represents the area/layer/level/zone like property of a routing protocol, such as an OSPF (area), IS-IS (layer) or PNNI (level). It does not represent the entire routing domain in every case. For example for OSPF, it represents an Area, but in the case of RIP, it represents the whole RIP domain. Any common attributes of these routing domains can be placed in this class in future versions of CIM.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_System
|
+--CIM_AdminDomain
|
+--CIM_RoutingProtocolDomain

## Direct Known Subclasses

CIM_OSPFArea

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | A Routing Protocol Domain is a collection of routers which coordinate their routing knowledge using a single [instance of a] routing protocol. This class represents the area/layer/level/zone like property of a routing protocol, such as an OSPF (area), IS-IS (layer) or PNNI (level). It does not represent the entire routing domain in every case. For example for OSPF, it represents an Area, but in the case of RIP, it represents the whole RIP domain. Any common attributes of these routing domains can be placed in this class in future versions of CIM.
UMLPackagePath | string | CIM::Network::RoutingForwarding
Version | string | 2.7.0

## Class Properties

### Inherited Properties

Name | Data Type
--- | ---
AllocationState | string
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
Name | string
NameFormat | string
OperatingStatus | uint16
OtherEnabledState | string
PrimaryOwnerContact | string
PrimaryOwnerName | string
PrimaryStatus | uint16
RequestedState | uint16
Status | string
TimeOfLastStateChange | datetime
TransitioningToState | uint16
AvailableRequestedStates | uint16[]
IdentifyingDescriptions | string[]
OperationalStatus | uint16[]
OtherIdentifyingInfo | string[]
Roles | string[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
RequestStateChange | uint32