# Class CIM_SNMPCommunityString
extends CIM_ServiceAccessPoint

SNMPCommunityString is an access point for an SNMPService. Each instance stores a community string that can be used for making SNMP requests.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_ServiceAccessPoint
|
+--CIM_SNMPCommunityString

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | SNMPCommunityString is an access point for an SNMPService. Each instance stores a community string that can be used for making SNMP requests.
UMLPackagePath | string | CIM::Network::SNMP
Version | string | 2.7.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
CommunityString | string |
Description | string | The SNMP community string/password used for read or read/write access to the agent's data.
MappingStrings | string | MIB.IETF|ENTITY-MIB.entLogicalCommunity
TypeOfAccess | uint16 |
Description | string | An enumerated integer describing whether read or read/ write access is granted, or whether this information is unknown.
ValueMap | string | 0, 1, 2
Values | string | Unknown, Read Only, Read/Write
LogicalEntitiesAccessed | string[] |
ArrayType | string | Indexed
Description | string | This array contains one or more object identifiers indicating the MIB modules/object subtrees that are accessed using the CommunityString. Either text strings of numbers (such as 1.2.3.4.5), or words (such as 'system') are specified. When using text strings of numbers, an asterisk (*) can replace any subidentifier to specify a subtree family - for example, 1.2.*.5. Descriptions related to each entry in the array are found at the corresponding index of the LogicalEntitiesDescriptions property.
MappingStrings | string | MIB.IETF|ENTITY-MIB.entLogicalType
ModelCorrespondence | string | CIM_SNMPCommunityString.LogicalEntitiesDescriptions
LogicalEntitiesDescriptions | string[] |
ArrayType | string | Indexed
Description | string | Free-form textual descriptions of the logical entities indicated in the LogicalEntitiesAccessed array. There is a correspondence between the entity identifier in the LogicalEntitiesAccessed array, and the description in this array at the corresponding index.
MappingStrings | string | MIB.IETF|ENTITY-MIB.entLogicalDescr
ModelCorrespondence | string | CIM_SNMPCommunityString.LogicalEntitiesAccessed

### Inherited Properties

Name | Data Type
--- | ---
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PrimaryStatus | uint16
RequestedState | uint16
Status | string
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TransitioningToState | uint16
AvailableRequestedStates | uint16[]
OperationalStatus | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
RequestStateChange | uint32