# Class CIM_TapePartition
extends CIM_MediaPartition

Capabilities and management of a TapePartition StorageExtent. Note that if a PhysicalTape is not partitioned, only a generic StorageExtent that represents the entire Tape should be instantiated. TapePartitions may be BasedOn other StorageExtents or directly Realized on a PhysicalTape.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_StorageExtent
|
+--CIM_MediaPartition
|
+--CIM_TapePartition

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Capabilities and management of a TapePartition StorageExtent. Note that if a PhysicalTape is not partitioned, only a generic StorageExtent that represents the entire Tape should be instantiated. TapePartitions may be BasedOn other StorageExtents or directly Realized on a PhysicalTape.
UMLPackagePath | string | CIM::Device::StorageExtents
Version | string | 2.6.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
NameFormat | uint16 | 1
Description | string | TapePartition names are application specific.
ModelCorrespondence | string | CIM_StorageExtent.Name, CIM_StorageExtent.NameNamespace, CIM_StorageExtent.OtherNameFormat
Override | string | NameFormat
ValueMap | string | 0, 1
Values | string | Other, Unknown
NameNamespace | uint16 | 1
Description | string | TapePartition names are application specific.
MappingStrings | string | SPC.INCITS-T10| VPD 83, Association 0 | Identifier
ModelCorrespondence | string | CIM_StorageExtent.Name, CIM_StorageExtent.OtherNameNamespace, CIM_StorageExtent.NameFormat
Override | string | NameNamespace
ValueMap | string | 0, 1
Values | string | Other, Unknown
UnusedBlocks | uint64 |
Description | string | Number of blocks that are currently unused/not written on the Partition. When this number is multiplied by the BlockSize, inherited from StorageExtent, the total number of bytes available for writing can be computed.
Gauge | boolean | true

### Inherited Properties

Name | Data Type
--- | ---
Access | uint16
Allocatable | boolean
AllocationState | string
Availability | uint16
BlockSize | uint64
Bootable | boolean
Caption | string
CommunicationStatus | uint16
CompressionRate | uint16
CompressionState | uint16
ConsumableBlocks | uint64
CreationClassName | string
DataOrganization | uint16
DataRedundancy | uint16
DeltaReservation | uint8
Description | string
DetailedStatus | uint16
DeviceID | string
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
ErrorCleared | boolean
ErrorDescription | string
ErrorMethodology | string
Extendable | boolean
ExtentInterleaveDepth | uint64
ExtentStripeLength | uint64
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
IsBasedOnUnderlyingRedundancy | boolean
IsComposite | boolean
IsCompressed | boolean
IsConcatenated | boolean
LastErrorCode | uint32
LocationIndicator | uint16
MaxQuiesceTime | uint64
Name | string
NoSinglePointOfFailure | boolean
NumberOfBlocks | uint64
OperatingStatus | uint16
OtherEnabledState | string
OtherNameFormat | string
OtherNameNamespace | string
OtherUsageDescription | string
PackageRedundancy | uint16
PowerManagementSupported | boolean
PowerOnHours | uint64
PrimaryStatus | uint16
Primordial | boolean
Purpose | string
RequestedState | uint16
SequentialAccess | boolean
Signature | string
SignatureAlgorithm | string
SignatureState | string
Status | string
StatusInfo | uint16
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TotalPowerOnHours | uint64
TransitioningToState | uint16
Usage | uint16
AdditionalAvailability | uint16[]
AvailableRequestedStates | uint16[]
ClientSettableUsage | uint16[]
ExtentDiscriminator | string[]
ExtentStatus | uint16[]
IdentifyingDescriptions | string[]
OperationalStatus | uint16[]
OtherIdentifyingInfo | string[]
PowerManagementCapabilities | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
EnableDevice | uint32
OnlineDevice | uint32
QuiesceDevice | uint32
RequestStateChange | uint32
Reset | uint32
RestoreProperties | uint32
SaveProperties | uint32
SetPowerState | uint32