# Class CIM_TelnetProtocolEndpoint
extends CIM_ProtocolEndpoint

A representation of a communications endpoint where a Telnet server can be accessed using the Telnet protocol.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_ServiceAccessPoint
|
+--CIM_ProtocolEndpoint
|
+--CIM_TelnetProtocolEndpoint

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | A representation of a communications endpoint where a Telnet server can be accessed using the Telnet protocol.
UMLPackagePath | string | CIM::Network::ConsoleProtocols
Version | string | 2.22.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
CharacterDisplayMode | uint16 |
Description | string | The character display mode that is currently active.
ModelCorrespondence | string | CIM_TelnetProtocolEndpoint.OtherCharacterDisplayMode, CIM_TelnetProtocolEndpoint.EnabledCharacterDisplayModes
ValueMap | string | 0, 1, 2, 3, 4..32767, 32768..65535
Values | string | Unknown, Other, Console, Stream, DMTF Reserved, Vendor Reserved
Write | boolean | true
EscapeCharacter | string |
Description | string | String indicating the Escape Character is in effect.
Write | boolean | true
IdleTimeout | uint32 | 0
Description | string | IdleTimeout specifies how long the connection can be idle before it is closed. The default value, 0, indicates that there is no idle timeout period.
PUnit | string | second
Units | string | Seconds
Write | boolean | true
OtherCharacterDisplayMode | string |
Description | string | When the CharacterDisplayMode property is set to 1, "Other" then this is a free form string providing more information about the character display mode. If not set to 1, this string has no meaning.
ModelCorrespondence | string | CIM_TelnetProtocolEndpoint.CharacterDisplayMode, CIM_TelnetProtocolEndpoint.OtherEnabledCharacterDisplayMode
Write | boolean | true
OtherTerminalMode | string |
Description | string | Where the TerminalMode property contains a value of 1, "Other" then this is a free form string providing more information about the current terminal mode and this value shall be one of the values in OtherEnabledTerminalModes. If not set to 1, this string has no meaning.
ModelCorrespondence | string | CIM_TelnetProtocolEndpoint.TerminalMode, CIM_TelnetProtocolEndpoint.OtherEnabledTerminalMode
Write | boolean | true
TerminalMode | uint16 |
Description | string | The terminal mode in use for this Telnet endpoint.This value shall be one of the values in EnabledTerminalModes
ModelCorrespondence | string | CIM_TelnetProtocolEndpoint.OtherTerminalMode, CIM_TelnetProtocolEndpoint.EnabledTerminalModes
ValueMap | string | 0, 1, 2, 3, 4..32767, 32768..65535
Values | string | Unknown, Other, VT100, ANSI, DMTF Reserved, Vendor Reserved
Write | boolean | true
EnabledCharacterDisplayModes | uint16[] |
ArrayType | string | Indexed
Description | string | An array of integers indicating the character display modes enabled for the service. Additional character display modes may be supported but currently not enabled for use.
ModelCorrespondence | string | CIM_TelnetProtocolEndpoint.OtherEnabledCharacterDisplayMode
ValueMap | string | 0, 1, 2, 3, 4..32767, 32768..65535
Values | string | Unknown, Other, Console, Stream, DMTF Reserved, Vendor Reserved
Write | boolean | true
EnabledTerminalModes | uint16[] |
ArrayType | string | Indexed
Description | string | An array of integers indicating the terminal modes that are enabled for use in this server connection. Additional terminal modes may be supported by the service but not enabled for use.
ModelCorrespondence | string | CIM_TelnetProtocolEndpoint.OtherEnabledTerminalMode
ValueMap | string | 0, 1, 2, 3, 4..32767, 32768..65535
Values | string | Unknown, Other, VT100, ANSI, DMTF Reserved, Vendor Reserved
OtherEnabledCharacterDisplayMode | string[] |
ArrayType | string | Indexed
Description | string | If the EnabledCharacterDisplayModes property is set to 1, "Other" then free form string providing more information about the enabled mode. If not set to 1, this string has no meaning.
ModelCorrespondence | string | CIM_TelnetProtocolEndpoint.EnabledCharacterDisplayModes
OtherEnabledTerminalMode | string[] |
ArrayType | string | Indexed
Description | string | If the EnabledTerminalModes property is set to 1, "Other" then free form string providing more information about supported terminal mode. If not set to 1, this string has no meaning.
ModelCorrespondence | string | CIM_TelnetProtocolEndpoint.EnabledTerminalModes

### Inherited Properties

Name | Data Type
--- | ---
BroadcastResetSupported | boolean
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
Name | string
NameFormat | string
OperatingStatus | uint16
OtherEnabledState | string
OtherTypeDescription | string
PrimaryStatus | uint16
ProtocolIFType | uint16
ProtocolType | uint16
RequestedState | uint16
Status | string
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TransitioningToState | uint16
AvailableRequestedStates | uint16[]
OperationalStatus | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
BroadcastReset | uint32
RequestStateChange | uint32