# Class CIM_TokenRingPort
extends CIM_NetworkPort

Capabilities and management of a TokenRingPort.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_LogicalPort
|
+--CIM_NetworkPort
|
+--CIM_TokenRingPort

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Capabilities and management of a TokenRingPort.
UMLPackagePath | string | CIM::Device::Ports
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
MaxDataSize | uint32 |
Description | string | The maximum size of the INFO (non-MAC) field that will be received or transmitted.
MappingStrings | string | MIB.IETF|BRIDGE-MIB.dot1dTpPortMaxInfo
RingOpenStatus | uint16 |
Description | string | This property indicates the success, or the reason for failure, of the most recent attempt by the station to enter the ring.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token Ring MIB.dot5RingOpenStatus
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10
Values | string | No Open Attempted, Bad Parameter, Lobe Failed, Signal Loss, Insertion Timeout, Ring Failed, Beaconing, Duplicate MAC, Request Failed, Remove Received, Last Open Successful
RingSpeed | uint16 |
Description | string | The bandwidth of the ring.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token Ring MIB.dot5RingSpeed
ValueMap | string | 0, 1, 2, 3, 4
Values | string | Unknown, Other, One Megabit, Four Megabit, Sixteen Megabit
RingState | uint16 |
Description | string | The current Device state with respect to entering or leaving the ring.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token Ring MIB.dot5RingState
ValueMap | string | 0, 1, 2, 3, 4, 5
Values | string | Opened, Closed, Opening, Closing, Open Failure, Ring Failure
RingStatus | uint32 |
Description | string | The current status that can be used to diagnose fluctuating problems that can occur on token rings, after a station has successfully been added to the ring. Before an open is completed, this object contains the value that indicates "no status" (131072). (The RingState and RingOpenStatus properties are also provided for debugging problems when the station cannot even enter the ring.) The value of the property is a sum of values, one for each currently applicable condition. The following values are defined for various conditions: 0 = No Problems Detected, 32 = Ring Recovery, 64 = Single Station, 256 = Remove Received, 512 = Reserved, 1024 = Auto-Removal Error, 2048 = Lobe Wire Fault, 4096 = Transmit Beacon, 8192 = Soft Error, 16384 = Hard Error, 32768 = Signal Loss, 131072 = No Status, Open Not Completed.
MappingStrings | string | MIB.IETF|IEEE 802.5 Token Ring MIB.dot5RingStatus
Capabilities | uint16[] |
ArrayType | string | Indexed
Description | string | Capabilities of the TokenRingPort. For example, the Device might support AlertOnLan, WakeOnLan, Load Balancing, or Failover. If failover or load balancing capabilities are listed, a SpareGroup (failover) or ExtraCapacityGroup (load balancing) should also be defined to completely describe the capability.
ModelCorrespondence | string | CIM_TokenRingPort.CapabilityDescriptions
ValueMap | string | 0, 1, 2, 3, 4, 5
Values | string | Unknown, Other, AlertOnLan, WakeOnLan, FailOver, LoadBalancing
CapabilityDescriptions | string[] |
ArrayType | string | Indexed
Description | string | An array of free-form strings that provides more detailed explanations for any of the TokenRingAPort features that are indicated in the Capabilities array. Note, each entry of this array is related to the entry in the Capabilities array that is located at the same index.
ModelCorrespondence | string | CIM_TokenRingPort.Capabilities
EnabledCapabilities | uint16[] |
ArrayType | string | Indexed
Description | string | Specifies which of the capabilities from the "Capabilities" property are currently enabled.
ModelCorrespondence | string | CIM_TokenRingPort.Capabilities, CIM_TokenRingPort.OtherEnabledCapabilities
ValueMap | string | 0, 1, 2, 3, 4, 5
Values | string | Unknown, Other, AlertOnLan, WakeOnLan, FailOver, LoadBalancing
NetworkAddresses | string[] |
Description | string | Token Ring/802.5 MAC addresses formatted as twelve hexadecimal digits (for example,"010203040506"), with each pair representing one of the six octets of the MAC address in "canonical" bit order. (Therefore, the Group address bit is found in the low order bit of the first character of the string.)
MappingStrings | string | MIF.DMTF|Network Adapter 802 Port|001.3
MaxLen | uint32 | 64
Override | string | NetworkAddresses
OtherEnabledCapabilities | string[] |
ArrayType | string | Indexed
Description | string | An array of free-form strings that provides more detailed explanations for any of the enabled capabilities that are specified as 'Other'.
ModelCorrespondence | string | CIM_TokenRingPort.EnabledCapabilities

### Inherited Properties

Name | Data Type
--- | ---
ActiveMaximumTransmissionUnit | uint64
AllocationState | string
AutoSense | boolean
Availability | uint16
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
DeviceID | string
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
ErrorCleared | boolean
ErrorDescription | string
FullDuplex | boolean
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LastErrorCode | uint32
LinkTechnology | uint16
LocationIndicator | uint16
MaxQuiesceTime | uint64
MaxSpeed | uint64
Name | string
OperatingStatus | uint16
OtherEnabledState | string
OtherLinkTechnology | string
OtherNetworkPortType | string
OtherPortType | string
PermanentAddress | string
PortNumber | uint16
PortType | uint16
PowerManagementSupported | boolean
PowerOnHours | uint64
PrimaryStatus | uint16
RequestedSpeed | uint64
RequestedState | uint16
Speed | uint64
Status | string
StatusInfo | uint16
SupportedMaximumTransmissionUnit | uint64
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TotalPowerOnHours | uint64
TransitioningToState | uint16
UsageRestriction | uint16
AdditionalAvailability | uint16[]
AvailableRequestedStates | uint16[]
IdentifyingDescriptions | string[]
OperationalStatus | uint16[]
OtherIdentifyingInfo | string[]
PowerManagementCapabilities | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
EnableDevice | uint32
OnlineDevice | uint32
QuiesceDevice | uint32
RequestStateChange | uint32
Reset | uint32
RestoreProperties | uint32
SaveProperties | uint32
SetPowerState | uint32