# Class CIM_VideoController
extends CIM_Controller

Note: The use of the CIM_VideoController class has been deprecated in lieu of CIM_DisplayController. Deprecated description: Capabilities and management of the VideoController.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_Controller
|
+--CIM_VideoController

## Direct Known Subclasses

CIM_AGPVideoController
CIM_PCVideoController

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Deprecated | string | CIM_DisplayController,CIM_VideoHead
Description | string | Note: The use of the CIM_VideoController class has been deprecated in lieu of CIM_DisplayController. Deprecated description: Capabilities and management of the VideoController.
UMLPackagePath | string | CIM::Device::Controller
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
CurrentBitsPerPixel | uint32 |
Deprecated | string | CIM_VideoHead.CurrentBitsPerPixel
Description | string | The number of bits used to display each pixel.
MappingStrings | string | MIF.DMTF|Video|004.12
PUnit | string | bit
Units | string | Bits
CurrentHorizontalResolution | uint32 |
Deprecated | string | CIM_VideoHead.CurrentHorizontalResolution
Description | string | Current number of horizontal pixels.
MappingStrings | string | MIF.DMTF|Video|004.11
PUnit | string | pixel
Units | string | Pixels
CurrentNumberOfColors | uint64 |
Deprecated | string | CIM_VideoHead.CurrentNumberOfColors
Description | string | The number of colors that are supported at the current resolutions.
CurrentNumberOfColumns | uint32 |
Deprecated | string | CIM_VideoHead.CurrentNumberOfColumns
Description | string | If in character mode, the number of columns for this VideoController. Otherwise, enter 0.
MappingStrings | string | MIF.DMTF|Video|004.14
CurrentNumberOfRows | uint32 |
Deprecated | string | CIM_VideoHead.CurrentNumberOfRows
Description | string | If in character mode, the number of rows for this Video Controller. Otherwise, enter 0.
MappingStrings | string | MIF.DMTF|Video|004.13
CurrentRefreshRate | uint32 |
Deprecated | string | CIM_VideoHead.CurrentRefreshRate
Description | string | Current refresh rate in hertz.
MappingStrings | string | MIF.DMTF|Video|004.15
PUnit | string | hertz
Units | string | Hertz
CurrentScanMode | uint16 |
Deprecated | string | CIM_VideoHead.CurrentScanMode
Description | string | Current scan mode. "Interlaced" (value=3) or "Non Interlaced" (value=4) can be defined using this property.
MappingStrings | string | MIF.DMTF|Video|004.8
ValueMap | string | 1, 2, 3, 4
Values | string | Other, Unknown, Interlaced, Non Interlaced
CurrentVerticalResolution | uint32 |
Deprecated | string | CIM_VideoHead.CurrentVerticalResolution
Description | string | Current number of vertical pixels.
MappingStrings | string | MIF.DMTF|Video|004.10
PUnit | string | pixel
Units | string | Pixels
Description | string |
Deprecated | string | No value
Description | string | The Description property provides a textual description of the object.
MappingStrings | string | MIF.DMTF|Video|004.18
Override | string | Description
MaxMemorySupported | uint32 |
Deprecated | string | CIM_DisplayController.MaxMemorySupported
Description | string | Maximum amount of memory supported in bytes.
PUnit | string | byte
Units | string | Bytes
MaxRefreshRate | uint32 |
Deprecated | string | CIM_VideoHead.MaxRefreshRate
Description | string | Maximum refresh rate of the VideoController in hertz.
MappingStrings | string | MIF.DMTF|Video|004.5
PUnit | string | hertz
Units | string | Hertz
MinRefreshRate | uint32 |
Deprecated | string | CIM_VideoHead.MinRefreshRate
Description | string | Minimum refresh rate of the Video Controller in hertz.
MappingStrings | string | MIF.DMTF|Video|004.4
PUnit | string | hertz
Units | string | Hertz
NumberOfVideoPages | uint32 |
Deprecated | string | CIM_DisplayController.NumberOfVideoPages
Description | string | Number of video pages that are supported given the current resolutions and available memory.
VideoMemoryType | uint16 |
Deprecated | string | CIM_DisplayController.VideoMemoryType
Description | string | An integer enumeration that indicates the type of video memory.
MappingStrings | string | MIF.DMTF|Video|004.6
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13
Values | string | Other, Unknown, VRAM, DRAM, SRAM, WRAM, EDO RAM, Burst Synchronous DRAM, Pipelined Burst SRAM, CDRAM, 3DRAM, SDRAM, SGRAM
VideoProcessor | string |
Deprecated | string | CIM_DisplayController.VideoProcessor
Description | string | A free-form string that describes the video processor or Controller.
AcceleratorCapabilities | uint16[] |
ArrayType | string | Indexed
Deprecated | string | CIM_DisplayController.AcceleratorCapabilities
Description | string | An array of integers that indicates the graphics and 3D capabilities of the VideoController.
ModelCorrespondence | string | CIM_VideoController.CapabilityDescriptions
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8
Values | string | Unknown, Other, Graphics Accelerator, 3D Accelerator, PCI Fast Write, MultiMonitor Support, PCI Mastering, Second Monochrome Adapter Support, Large Memory Address Support
CapabilityDescriptions | string[] |
ArrayType | string | Indexed
Deprecated | string | CIM_DisplayController.CapabilityDescriptions
Description | string | An array of free-form strings that provides more detailed explanations for any of the video Accelerator features that are indicated in the Capabilities array. Note, each entry of this array is related to the entry in the Capabilities array that is located at the same index.
ModelCorrespondence | string | CIM_VideoController.AcceleratorCapabilities

### Inherited Properties

Name | Data Type
--- | ---
AllocationState | string
Availability | uint16
Caption | string
CommunicationStatus | uint16
CreationClassName | string
DetailedStatus | uint16
DeviceID | string
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
ErrorCleared | boolean
ErrorDescription | string
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LastErrorCode | uint32
LocationIndicator | uint16
MaxNumberControlled | uint32
MaxQuiesceTime | uint64
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PowerManagementSupported | boolean
PowerOnHours | uint64
PrimaryStatus | uint16
ProtocolDescription | string
ProtocolSupported | uint16
RequestedState | uint16
Status | string
StatusInfo | uint16
SystemCreationClassName | string
SystemName | string
TimeOfLastReset | datetime
TimeOfLastStateChange | datetime
TotalPowerOnHours | uint64
TransitioningToState | uint16
AdditionalAvailability | uint16[]
AvailableRequestedStates | uint16[]
IdentifyingDescriptions | string[]
OperationalStatus | uint16[]
OtherIdentifyingInfo | string[]
PowerManagementCapabilities | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
EnableDevice | uint32
OnlineDevice | uint32
QuiesceDevice | uint32
RequestStateChange | uint32
Reset | uint32
RestoreProperties | uint32
SaveProperties | uint32
SetPowerState | uint32