# Class CIM_DiagnosticLog
extends CIM_RecordLog

DiagnosticLog serves as an aggregation point for DiagnosticRecord objects. This class exists in order to encourage the use of a consolidated record management methodology for diagnostics. A common set of providers for this log and its associated records SHOULD be used to control functions such as record persistence, query support and overall data integrity in a consistent manner.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Log
|
+--CIM_RecordLog
|
+--CIM_DiagnosticLog

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | DiagnosticLog serves as an aggregation point for DiagnosticRecord objects. This class exists in order to encourage the use of a consolidated record management methodology for diagnostics. A common set of providers for this log and its associated records SHOULD be used to control functions such as record persistence, query support and overall data integrity in a consistent manner.
UMLPackagePath | string | CIM::System::Logs
Version | string | 2.22.0

## Class Properties

### Inherited Properties

Name | Data Type
--- | ---
Caption | string
CommunicationStatus | uint16
CurrentNumberOfRecords | uint64
Description | string
DetailedStatus | uint16
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LogState | uint16
MaxNumberOfRecords | uint64
Name | string
OperatingStatus | uint16
OtherEnabledState | string
OverwritePolicy | uint16
PrimaryStatus | uint16
RequestedState | uint16
Status | string
TimeOfLastStateChange | datetime
TransitioningToState | uint16
AvailableRequestedStates | uint16[]
OperationalStatus | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
ClearLog | uint32
RequestStateChange | uint32