# Class CIM_SourceRoutingService
extends CIM_ForwardingService

SourceRoutingService represents the capability of a switch to participate in the source routing of frames received at its ports. It is a system-level Service that provides and supports local switching only. The SourceRouting Service is aggregated into a higher level SwitchService through the SwitchServiceSourceRouting association.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_NetworkService
|
+--CIM_ForwardingService
|
+--CIM_SourceRoutingService

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | SourceRoutingService represents the capability of a switch to participate in the source routing of frames received at its ports. It is a system-level Service that provides and supports local switching only. The SourceRouting Service is aggregated into a higher level SwitchService through the SwitchServiceSourceRouting association.
UMLPackagePath | string | CIM::Network::SwitchingBridging
Version | string | 2.7.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
BridgeLfMode | uint16 |
Description | string | Indicates whether the bridge operates using older 3 bit length negotiation fields or the newer 6 bit length field in its RIF.
MappingStrings | string | MIB.IETF|SOURCE-ROUTING-MIB.dot1dSrBridgeLfMode
ValueMap | string | 1, 2
Values | string | Mode3, Mode6

### Inherited Properties

Name | Data Type
--- | ---
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LoSID | string
LoSOrgID | string
Name | string
OperatingStatus | uint16
OtherEnabledState | string
OtherProtocolType | string
PrimaryOwnerContact | string
PrimaryOwnerName | string
PrimaryStatus | uint16
ProtocolType | uint16
RequestedState | uint16
ServiceURL | string
Started | boolean
StartMode | string
Status | string
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TransitioningToState | uint16
AvailableRequestedStates | uint16[]
Keywords | string[]
OperationalStatus | uint16[]
StartupConditions | string[]
StartupParameters | string[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
ChangeAffectedElementsAssignedSequence | uint32
RequestStateChange | uint32
StartService | uint32
StopService | uint32