# Class CIM_Door
extends CIM_LogicalDevice

A Door is the abstraction of hardware providing access to the internal componentry of a System. When a Door is 'opened', typically all accessible, moving components are stopped or suspended to prevent physical harm.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_Door

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | A Door is the abstraction of hardware providing access to the internal componentry of a System. When a Door is 'opened', typically all accessible, moving components are stopped or suspended to prevent physical harm.
UMLPackagePath | string | CIM::Device::UserDevices
Version | string | 2.6.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
LastOpened | datetime |
Description | string | Date and time that the Door was last opened.
Locked | boolean |
Description | string | Boolean indicating that the Door is 'locked' (TRUE) or 'unlocked' (FALSE). When the Door is locked, access to the componentry is prevented, without the use of a physical key or the issuance of a software unlock command.
Open | boolean |
Description | string | Boolean indicating the 'open' (TRUE) or 'closed' (FALSE) status of the Door.
Timeout | uint32 |
Description | string | When a Door is 'Open', all accessible, moving componentry and Device operation are typically stopped. The Timeout property provides a mechanism to event on a Door left open for a period of time (in seconds) exceeding the property's value.
PUnit | string | second
Units | string | Seconds
Capabilities | uint16[] |
Description | string | The Capabilities of the Door. For example, information on whether the Door is "Host System Lockable" (value=2) and/or whether a key is available (value=3) are specified in this property. The value 4, "All Drives Dismounted Before Access", pertains to a Door on a StorageLibrary or set of drive bays. If specified for the Door, it means that it can not be opened unless all Media are first unloaded from the accessible MediaAccessDevices.
ValueMap | string | 0, 1, 2, 3, 4
Values | string | Unknown, Other, Host System Lockable, Physical Key, All Drives Dismounted Before Access

### Inherited Properties

Name | Data Type
--- | ---
AllocationState | string
Availability | uint16
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
DeviceID | string
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
ErrorCleared | boolean
ErrorDescription | string
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LastErrorCode | uint32
LocationIndicator | uint16
MaxQuiesceTime | uint64
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PowerManagementSupported | boolean
PowerOnHours | uint64
PrimaryStatus | uint16
RequestedState | uint16
Status | string
StatusInfo | uint16
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TotalPowerOnHours | uint64
TransitioningToState | uint16
AdditionalAvailability | uint16[]
AvailableRequestedStates | uint16[]
IdentifyingDescriptions | string[]
OperationalStatus | uint16[]
OtherIdentifyingInfo | string[]
PowerManagementCapabilities | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
EnableDevice | uint32
OnlineDevice | uint32
QuiesceDevice | uint32
RequestStateChange | uint32
Reset | uint32
RestoreProperties | uint32
SaveProperties | uint32
SetPowerState | uint32