# Class CIM_MemoryConfigurationService
extends CIM_Service

Instances of the CIM_MemoryConfigurationService exist to facilitate provisioning of system memory. Traditionally the platform BIOS is able to map memory resources into the system address space without user intervention. Some memory devices may support or require configuration prior to being made available in the system address space. The CIM_MemoryConfigurationService is utilized with this later type of memory device. It supports allocation, a process by which primordial, unconfigured memory is made available to the system. It also supports deallocation, whereby visible extents are returned to their primordial state.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_MemoryConfigurationService

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Instances of the CIM_MemoryConfigurationService exist to facilitate provisioning of system memory. Traditionally the platform BIOS is able to map memory resources into the system address space without user intervention. Some memory devices may support or require configuration prior to being made available in the system address space. The CIM_MemoryConfigurationService is utilized with this later type of memory device. It supports allocation, a process by which primordial, unconfigured memory is made available to the system. It also supports deallocation, whereby visible extents are returned to their primordial state.
UMLPackagePath | string | CIM::Device::ConfigurableMemory
Version | string | 2.47.0

## Class Properties

### Inherited Properties

Name | Data Type
--- | ---
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LoSID | string
LoSOrgID | string
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PrimaryOwnerContact | string
PrimaryOwnerName | string
PrimaryStatus | uint16
RequestedState | uint16
Started | boolean
StartMode | string
Status | string
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TransitioningToState | uint16
AvailableRequestedStates | uint16[]
OperationalStatus | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
ChangeAffectedElementsAssignedSequence | uint32
RequestStateChange | uint32
StartService | uint32
StopService | uint32