# Class CIM_FCSwitchCapabilities
extends CIM_EnabledLogicalElementCapabilities

FibreChannel switch control and configuration capabilities.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_Capabilities
|
+--CIM_EnabledLogicalElementCapabilities
|
+--CIM_FCSwitchCapabilities

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | FibreChannel switch control and configuration capabilities.
UMLPackagePath | string | CIM::Device::FC
Version | string | 2.45.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
DomainIDConfigureable | boolean |
Description | string | Boolean that indicates whether the DomainID setting can be modified.
MappingStrings | string | FC-SWAPI.INCITS-T11|SWAPI_UNIT_CONFIG_CAPS_T|EditDomainID
ModelCorrespondence | string | CIM_FCSwitchSettings.PreferredDomainID
DomainIDLockedSupported | boolean |
Description | string | Boolean that indicates whether the DomainIDLocked setting can be modified.
MappingStrings | string | FC-SWAPI.INCITS-T11|SWAPI_UNIT_CONFIG_CAPS_T|EditDomainIDLocked
ModelCorrespondence | string | CIM_FCSwitchSettings.DomainIDLocked
MaxDomainID | uint8 |
Description | string | Maximum DomainID value supported by the switch. This value must be greater than or equal to MinDomainID.
MappingStrings | string | FC-SWAPI.INCITS-T11|SWAPI_UNIT_CONFIG_CAPS_T|MaxDomainID
MaxValue | sint64 | 239
MinValue | sint64 | 1
ModelCorrespondence | string | CIM_FCSwitchSettings.PreferredDomainID
MinDomainID | uint8 |
Description | string | Minimum DomainID value supported by the switch.
MappingStrings | string | FC-SWAPI.INCITS-T11|SWAPI_UNIT_CONFIG_CAPS_T|MinDomainID
MaxValue | sint64 | 239
MinValue | sint64 | 1
ModelCorrespondence | string | CIM_FCSwitchSettings.PreferredDomainID
NPIVSupported | boolean |
Description | string | Flag indicating whether NPIV is supported on the fibre channel switch.
PrincipalPrioritiesSupported | uint16[] |
Description | string | This array contains the principal priority settings that are supported by the switch.
MappingStrings | string | FC-SWAPI.INCITS-T11|SWAPI_UNIT_CONFIG_CAPS_T|SupportedSwitchPriorities
ModelCorrespondence | string | CIM_FCSwitchSettings.PrincipalPriority
ValueMap | string | 2, 3, 4, 5
Values | string | Principal, Subordinate, Any, Not Applicable

### Inherited Properties

Name | Data Type
--- | ---
Caption | string
Description | string
ElementName | string
ElementNameEditSupported | boolean
ElementNameMask | string
Generation | uint64
InstanceID | string
MaxElementNameLen | uint16
RequestedStatesSupported | uint16[]
StateAwareness | uint16[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
CreateGoalSettings | uint16