# Class CIM_VLANService
extends CIM_Service

This class is deprecated following discussion as to the need of a modeling a VLAN as a service. It was determined that a VLAN service was not needed. VLANService represents the VLAN aspects of the function performed by a switch. Some VLAN-aware devices participate in protocols where VLAN information is propagated among switches, e.g., GVRP in 802.1Q switches and VTP in Cisco Catalyst switches. VLANService also represents the function performed by the switch as a participant in such a protocol. VLANService must be subclassed so that the type of instance can be distinguished by its class.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_VLANService

## Direct Known Subclasses

CIM_Specific802dot1QVLANService

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Abstract | boolean | true
Deprecated | string | No value
Description | string | This class is deprecated following discussion as to the need of a modeling a VLAN as a service. It was determined that a VLAN service was not needed. VLANService represents the VLAN aspects of the function performed by a switch. Some VLAN-aware devices participate in protocols where VLAN information is propagated among switches, e.g., GVRP in 802.1Q switches and VTP in Cisco Catalyst switches. VLANService also represents the function performed by the switch as a participant in such a protocol. VLANService must be subclassed so that the type of instance can be distinguished by its class.
UMLPackagePath | string | CIM::Network::VLAN
Version | string | 2.8.0

## Class Properties

### Inherited Properties

Name | Data Type
--- | ---
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LoSID | string
LoSOrgID | string
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PrimaryOwnerContact | string
PrimaryOwnerName | string
PrimaryStatus | uint16
RequestedState | uint16
Started | boolean
StartMode | string
Status | string
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TransitioningToState | uint16
AvailableRequestedStates | uint16[]
OperationalStatus | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
ChangeAffectedElementsAssignedSequence | uint32
RequestStateChange | uint32
StartService | uint32
StopService | uint32