# Class CIM_BootSourceSetting
extends CIM_SettingData

A class derived from SettingData that provides the information necessary to describe a boot source. This may be optionally associated to a bootable logical device, such as a hard disk partition, or a network device. The information from this class instance is used by the boot manager, such as BIOS/EFI or OS Loader to initiate the boot process, when this instance appears in a BootConfigSetting collection.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_SettingData
|
+--CIM_BootSourceSetting

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | A class derived from SettingData that provides the information necessary to describe a boot source. This may be optionally associated to a bootable logical device, such as a hard disk partition, or a network device. The information from this class instance is used by the boot manager, such as BIOS/EFI or OS Loader to initiate the boot process, when this instance appears in a BootConfigSetting collection.
UMLPackagePath | string | CIM::System::Boot
Version | string | 2.19.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
BIOSBootString | string |
Description | string | A string identifying the boot source which corresponds to the string used by the BIOS to uniquely name the boot source. For example, in systems which implement the BIOS Boot Specification, the string could correspond to the descString string for entries in the IPL Table or BCV Table.
BootString | string |
Description | string | A string identifying the boot source. It is typically used by the instrumentation to pass to the boot manager as a selection string. This could be a string identifying the bootable device, such as "CDROM 1", or could be an implementation specific address of a bootable partition, such as the following. "fd(64)unix root=hd(40) swap=hd(41)", or "multi(0)disk(0)rdisk(0)partition(1)\WINDOWS="Microsoft Windows XP Professional"".
FailThroughSupported | uint16 |
Description | string | An enumeration indicating the behavior when the attempt to boot using the boot source fails (no media, timeout). The current values in the enumeration are: 0 = Unknown 1 = Is Supported 2 = Is Not Supported. A value of 1 (Is Supported) indicates that next boot source the boot order is used. A value of 2 (Is Not Supported) indicates that the boot order is terminated and no other boot sources associated to the same CIM_BootConfigSetting are used). The default is 1 (Is Supported)
ValueMap | string | 0, 1, 2
Values | string | Unknown, Is Supported, Not Supported
StructuredBootString | string |
Description | string | A string identifying the boot source using the format "<OrgID>:<identifier>:<index>", in which neither <OrgID>, <identifier> or <index> contains a colon (":"). The value of <OrgID> is a copyrighted, trademarked or otherwise unique name that is owned by the entity defining the <identifier>, or is a registered ID that is assigned to the entity by a recognized global authority. For DMTF defined identifiers, the <OrgID> is set to 'CIM'. The <identifiers> are "Floppy", "Hard-Disk", "CD/DVD", "Network", "PCMCIA", "USB". The value of <index> shall be a non-zero integer.

### Inherited Properties

Name | Data Type
--- | ---
Caption | string
ChangeableType | uint16
ConfigurationName | string
Description | string
ElementName | string
Generation | uint64
InstanceID | string
SoID | string
SoOrgID | string
ComponentSetting | string[]

## Class Methods