# Class CIM_WiFiPort
extends CIM_NetworkPort

WiFiPort is the logical representation of wireless local area network communications hardware that conforms to the IEEE 802.11 series of specifications. It embodies properties at the lowest layers of a network stack, such as the antennas used for transmission and reception, the address permanently embedded into the hardware, and the operational bandwidth of the device.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_LogicalPort
|
+--CIM_NetworkPort
|
+--CIM_WiFiPort

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | WiFiPort is the logical representation of wireless local area network communications hardware that conforms to the IEEE 802.11 series of specifications. It embodies properties at the lowest layers of a network stack, such as the antennas used for transmission and reception, the address permanently embedded into the hardware, and the operational bandwidth of the device.
UMLPackagePath | string | CIM::Device::Ports
Version | string | 2.22.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
MaxSpeed | uint64 |
Description | string | Shall contain the maximum bandwidth relative to the current operating mode specified in PortType. For example, shall contain 11000000 if PortType contains 71 ("802.11b").
Override | string | MaxSpeed
PUnit | string | bit / second
Units | string | Bits per Second
PermanentAddress | string |
Description | string | IEEE 802 EUI-48 MAC address, formatted as twelve hexadecimal digits (for example, "010203040506"), with each pair representing one of the six octets of the MAC address in "canonical" bit order. (Therefore, the Group address bit is found in the low order bit of the first character of the string.)
MappingStrings | string | MIF.DMTF|Network Adapter 802 Port|001.2
MaxLen | uint32 | 64
Override | string | PermanentAddress
PortType | uint16 |
Description | string | PortType shall contain the specific 802.11 operating mode that is currently enabled on the Port. All modes are specified in
ModelCorrespondence | string | CIM_NetworkPort.OtherNetworkPortType
Override | string | PortType
ValueMap | string | 0, 1, 70, 71, 72, 73, .., 16000..
Values | string | Unknown, Other, 802.11a, 802.11b, 802.11g, 802.11n, DMTF Reserved, Vendor Reserved
Speed | uint64 |
Description | string | The data rate at which the current PPDU (PLCP (Physical Layer Convergence Protocol) Protocol Data Unit) was received. This value is encoded in the first 4 bits of the PLCP header in each PLCP frame.
MappingStrings | string | MIB.IETF|MIB-II.ifSpeed, MIF.DMTF|Network Adapter 802 Port|001.5
Override | string | Speed
PUnit | string | bit / second
Units | string | Bits per Second
NetworkAddresses | string[] |
Description | string | IEEE 802 EUI-48 MAC addresses, each formatted as twelve hexadecimal digits (for example, "010203040506"), with each pair representing one of the six octets of the MAC address in "canonical" bit order. (Therefore, the Group address bit is found in the low order bit of the first character of the string.)
MappingStrings | string | MIF.DMTF|Network Adapter 802 Port|001.3
MaxLen | uint32 | 64
Override | string | NetworkAddresses

### Inherited Properties

Name | Data Type
--- | ---
ActiveMaximumTransmissionUnit | uint64
AllocationState | string
AutoSense | boolean
Availability | uint16
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
DeviceID | string
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
ErrorCleared | boolean
ErrorDescription | string
FullDuplex | boolean
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LastErrorCode | uint32
LinkTechnology | uint16
LocationIndicator | uint16
MaxQuiesceTime | uint64
Name | string
OperatingStatus | uint16
OtherEnabledState | string
OtherLinkTechnology | string
OtherNetworkPortType | string
OtherPortType | string
PortNumber | uint16
PowerManagementSupported | boolean
PowerOnHours | uint64
PrimaryStatus | uint16
RequestedSpeed | uint64
RequestedState | uint16
Status | string
StatusInfo | uint16
SupportedMaximumTransmissionUnit | uint64
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TotalPowerOnHours | uint64
TransitioningToState | uint16
UsageRestriction | uint16
AdditionalAvailability | uint16[]
AvailableRequestedStates | uint16[]
IdentifyingDescriptions | string[]
OperationalStatus | uint16[]
OtherIdentifyingInfo | string[]
PowerManagementCapabilities | uint16[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
EnableDevice | uint32
OnlineDevice | uint32
QuiesceDevice | uint32
RequestStateChange | uint32
Reset | uint32
RestoreProperties | uint32
SaveProperties | uint32
SetPowerState | uint32