# Class CIM_BGPService
extends CIM_RouteCalculationService

This class is used to represent the basic operation of BGP. It is derived from RouteCalculationService, the superclass of all routing protocols.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_NetworkService
|
+--CIM_RouteCalculationService
|
+--CIM_BGPService

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class is used to represent the basic operation of BGP. It is derived from RouteCalculationService, the superclass of all routing protocols.
UMLPackagePath | string | CIM::Network::BGP
Version | string | 2.7.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
BGPVersion | uint8 |
Description | string | The BGPVersion property defines the version of BGP that this router is using. This is part of the BGP peer negotiation process).
MappingStrings | string | MIB.IETF|BGP4-MIB.bgpVersion
LastErrorCode | uint16 |
Description | string | BGP sends errors using a NOTIFICATION message. This message contains an error code, an error subcode, and error data. The error code defines the type of the notification. The 'Cease' error is for all fatal errors that are not one of the other five types of errors. For several of the errors, subcode information is also enumerated in other properties of this class.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6
Values | string | None, Message Header Error, OPEN Message Error, UPDATE Message Error, Hold Timer Expired, Finite State Machine Error, Cease
LastMessageErrorSubCode | uint16 |
Description | string | This defines the BGP error subcode for message header errors (LastErrorCode = 1). If LastErrorCode is any other value, then this property should be set to NULL.
ValueMap | string | 0, 1, 2, 3
Values | string | None, Connection Not Synchronized, Bad Message Length, Bad Message Type
LastOpenErrorSubCode | uint16 |
Description | string | This defines the BGP error subcode for OPEN message errors (LastErrorCode = 2). If LastErrorCode is any other value, then this property should be set to NULL.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6
Values | string | None, Unsupported Version Number, Bad Peer AS, Bad BGP Identifier, Unsupported Optional Parameter, Authentication Failure, Unacceptable Hold Time
LastUpdateErrorSubCode | uint16 |
Description | string | This defines the BGP error subcode for UPDATE message errors (LastErrorCode = 3). If LastErrorCode is any other value, then this property should be set to NULL.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11
Values | string | None, Malformed Attribute List, Unrecognized Well-Known Attribute, Missing Well-Known Attribute, Attribute Flags Error, Attribute Length Error, Invalid Origin Attribute, AS Routing Loop, Invalid NEXT_HOP Attribute, Optional Attribute Error, Invalid Network Field, Malformed AS_path

### Inherited Properties

Name | Data Type
--- | ---
AlgorithmType | uint16
Caption | string
CommunicationStatus | uint16
CreationClassName | string
Description | string
DetailedStatus | uint16
ElementName | string
EnabledDefault | uint16
EnabledState | uint16
Generation | uint64
HealthState | uint16
InstallDate | datetime
InstanceID | string
LoSID | string
LoSOrgID | string
Name | string
OperatingStatus | uint16
OtherEnabledState | string
PrimaryOwnerContact | string
PrimaryOwnerName | string
PrimaryStatus | uint16
RequestedState | uint16
RouterID | string
ServiceURL | string
Started | boolean
StartMode | string
Status | string
SystemCreationClassName | string
SystemName | string
TimeOfLastStateChange | datetime
TransitioningToState | uint16
AvailableRequestedStates | uint16[]
Keywords | string[]
OperationalStatus | uint16[]
StartupConditions | string[]
StartupParameters | string[]
StatusDescriptions | string[]

## Class Methods

### Inherited Class Methods

Name | Return Type
--- | ---
ChangeAffectedElementsAssignedSequence | uint32
RequestStateChange | uint32
StartService | uint32
StopService | uint32