# Class CIM_ImagingMediaUsedStatisticalData
extends CIM_ImagingStatisticalData

This class defines media used (for accounting and billing) ImagingStatisticalData associated with an imaging system (e.g., ComputerSystem), imaging service (e.g., PrintService), imaging device (e.g., Printer), imaging job (e.g., PrintJob), or any other imaging element. See: Section 4 Overview in PWG Counter MIB v2 (PWG 5106.3).

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_StatisticalData
|
+--CIM_ImagingStatisticalData
|
+--CIM_ImagingMediaUsedStatisticalData

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class defines media used (for accounting and billing) ImagingStatisticalData associated with an imaging system (e.g., ComputerSystem), imaging service (e.g., PrintService), imaging device (e.g., Printer), imaging job (e.g., PrintJob), or any other imaging element. See: Section 4 Overview in PWG Counter MIB v2 (PWG 5106.3).
Experimental | boolean | true
UMLPackagePath | string | CIM::Core::Statistics
Version | string | 2.20.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
BlankSheets | uint32 |
Description | string | Blank sheets of this specific media printed by this managed element (e.g., PrintService or PrintMarker).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icMediaUsedBlankSheets
FullColorSheets | uint32 |
Description | string | Full color sheets of this specific media printed by this managed element (e.g., PrintService or PrintMarker).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icMediaUsedFullColorSheets
HighlightColorSheets | uint32 |
Description | string | Highlight color sheets of this specific media printed by this managed element (e.g., PrintService or PrintMarker).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icMediaUsedHighlightColorSheets
MediaAccountingKey | string |
Description | string | The locally unique accounting key for this specific media, for use with remote accounting systems, network management systems, fleet management based on SLAs (service level agreements), etc., specified as a visible US-ASCII string (ANSI X.3-1968) that shall not contain any US-ASCII control characters (0x00 to 0x1F inclusive, or 0x7F). This locally unique media accounting key may be specified in any natural language that can be represented in or transliterated into US-ASCII, but shall not be localized. This media accounting key should conform to the ABNF in Appendix A Media Accounting Key Format of PWG 5106.3 for interoperability. This media accounting key may contain characters not permitted in IPP keyword or name datatypes, unlike the corresponding (but more restricted) IPP media-key attribute defined in IPP Production Printing Set1 (IEEE/ISTO PWG 5100.3).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icMediaUsedMediaAccountingKey
MaxLen | uint32 | 255
MinLen | uint32 | 0
MediaInfo | string |
Description | string | The localized description of this specific media, for use with remote network management scripts and GUIs, specified as a Unicode string in the locale of the scoping managed element (e.g., CIM_Printer.CurrentNaturalLanguage). For example: Light blue deckle-edge letter stock. This media description should clearly distinguish different instances of the same media size (for example, by including specific media color, weight, etc.).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icMediaUsedMediaInfo
MaxLen | uint32 | 255
MinLen | uint32 | 0
MediaName | string |
Description | string | The friendly locally unique name for this specific media, for use with remote network management scripts and GUIs, specified as a Unicode string. This locally unique media name may be specified in any natural language, but shall not be localized. For example: customer-reply or na-letter-colored. Note: PWG Media Standardized Names (PWG 5101.1) restricts even custom media names to use US-ASCII strings (ANSI X.3-1968), although they may be specified in any natural language that can be represented in or transliterated into a US-ASCII string. On the other hand, IPP/1.1 (RFC 2911) and Job Mon MIB (RFC 2707) allow custom media names to use UTF-8 strings (RFC 3629).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icMediaUsedMediaName
MaxLen | uint32 | 255
MinLen | uint32 | 0
MediaSizeName | string |
Description | string | The media size self-describing name for this specific media, for use with remote network management scripts and GUIs, specified as a visible US-ASCII string (ANSI X.3-1968) that shall not contain any US-ASCII control characters (0x00 to 0x1F inclusive, or 0x7F). This media size name shall not be localized. For example: na_letter_8.5x11in.
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icMediaUsedMediaSizeName
MaxLen | uint32 | 255
MinLen | uint32 | 0
MonochromeSheets | uint32 |
Description | string | Monochrome sheets of this specific media printed by this managed element (e.g., PrintService or PrintMarker).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icMediaUsedMonochromeSheets
SNMPRowId | uint32 |
Description | string | A unique value used by the scoping imaging element (e.g., PrintService) to identify this instance of specific media. Note: This property is necessary to correlate counter and event information between CIM and SNMP interfaces.
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icMediaUsedIndex
MaxValue | sint64 | 2147483647
MinValue | sint64 | 1
TotalSheets | uint32 |
Description | string | Total sheets of this specific media printed by this managed element (e.g., PrintService or PrintMarker).
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icMediaUsedTotalSheets

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
Description | string | CIM_ManagedElement
ElementName | string | CIM_StatisticalData
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_StatisticalData
OtherPersistenceType | string | CIM_ImagingStatisticalData
PersistenceType | uint16 | CIM_ImagingStatisticalData
SampleInterval | datetime | CIM_StatisticalData
SNMPKeyId | uint32 | CIM_ImagingStatisticalData
StartStatisticTime | datetime | CIM_StatisticalData
StatisticTime | datetime | CIM_StatisticalData

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ResetSelectedStats | uint32 | CIM_StatisticalData