# Class CIM_BlockStatisticsManifest
extends CIM_ManagedElement

Instances of this class define a list of supported or desired properties of BlockStatisticalData instances. In the case where a BlockStatisticsManifest instance is a member of a BlockStatisticsManifestCollection used in a BlockStatisticsService.GetStatisticsCollection request, for each of the boolean "include" properties set to true in that BlockStatisticsManifest, the corresponding BlockStatisticalData property will be included, if available, in the statistics returned for BlockStatisticalData instances whose ElementType matches the ElementType of the BlockStatisticsManifest.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_BlockStatisticsManifest

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Instances of this class define a list of supported or desired properties of BlockStatisticalData instances. In the case where a BlockStatisticsManifest instance is a member of a BlockStatisticsManifestCollection used in a BlockStatisticsService.GetStatisticsCollection request, for each of the boolean "include" properties set to true in that BlockStatisticsManifest, the corresponding BlockStatisticalData property will be included, if available, in the statistics returned for BlockStatisticalData instances whose ElementType matches the ElementType of the BlockStatisticsManifest.
UMLPackagePath | string | CIM::Device::StorageStatistics
Version | string | 2.28.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
ElementType | uint16 |
Description | string | Determines the type of elements that this BlockStatisticsManifest can be applied to (e.g. during a GetStatisticsCollection request). This is used when the same set of statistical metrics is calculated for several types of devices. In this way, a single BlockStatisticsManifest instance can be used to filter all the StatsiticalData instances that contain metrics for the same type of element in a StatisticsCollection. If used, a subclass should override this property to specify the element types supported by that class, preferably through ValueMap and Values qualifiers to allow clients to programmatically retrieve those supported types.
ModelCorrespondence | string | CIM_BlockStorageStatisticalData.ElementType
ValueMap | string | 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, .., 0x8000..
Values | string | Computer System, Front-end Computer System, Peer Computer System, Back-end Computer System, Front-end Port, Back-end Port, Volume, Extent, Disk Drive, Arbitrary LUs, Remote Replica Group, DMTF Reserved, Vendor Specific
IncludeIdleTimeCounter | boolean | false
Description | string | Whether to include in a filter for a metered element the cumulative elapsed idle time for that element.
ModelCorrespondence | string | CIM_BlockStorageStatisticalData.IdleTimeCounter
IncludeIOTimeCounter | boolean | false
Description | string | Whether to include in a filter for a metered element the cumulative elapsed I/O time (number of Clock Tick Intervals) for all I/Os for that element as defined in 'Total I/Os'.
ModelCorrespondence | string | CIM_BlockStorageStatisticalData.IOTimeCounter
IncludeKBytesRead | boolean | false
Description | string | Whether to include in a filter for a metered element the cumulative count of data read in Kbytes for that element.
ModelCorrespondence | string | CIM_BlockStorageStatisticalData.KBytesRead
IncludeKBytesTransferred | boolean | false
Description | string | Whether to include in a filter for a metered element the cumulative count of data transferred in Kbytes for that element.
ModelCorrespondence | string | CIM_BlockStorageStatisticalData.KBytesTransferred
IncludeKBytesWritten | boolean | false
Description | string | Whether to include in a filter for a metered element the cumulative count of data written in Kbytes for that element.
ModelCorrespondence | string | CIM_BlockStorageStatisticalData.KBytesWritten
IncludeMaintOp | boolean | false
Description | string | Whether to include in a filter for a metered element the cumulative count of all maintenance operations for that element.
ModelCorrespondence | string | CIM_BlockStorageStatisticalData.MaintOp
IncludeMaintTimeCounter | boolean | false
Description | string | Whether to include in a filter for a metered element the cumulative elapsed maintenance time for that element.
ModelCorrespondence | string | CIM_BlockStorageStatisticalData.MaintTimeCounter
IncludeReadHitIOs | boolean | false
Description | string | Whether to include in a filter for a metered element the cumulative count of all read cache hits (Reads from Cache) for that element.
ModelCorrespondence | string | CIM_BlockStorageStatisticalData.ReadHitIOs
IncludeReadHitIOTimeCounter | boolean | false
Description | string | Whether to include in a filter for a metered element the cumulative elapsed time for all Read I/Os read from cache for that element.
ModelCorrespondence | string | CIM_BlockStorageStatisticalData.ReadHitIOTimeCounter
IncludeReadIOs | boolean | false
Description | string | Whether to include in a filter for a metered element the cumulative count of all reads for that element.
ModelCorrespondence | string | CIM_BlockStorageStatisticalData.ReadIOs
IncludeReadIOTimeCounter | boolean | false
Description | string | Whether to include in a filter for a metered element the cumulative elapsed time for all cumulative Read I/Os for that element.
ModelCorrespondence | string | CIM_BlockStorageStatisticalData.ReadIOTimeCounter
IncludeStartStatisticTime | boolean | false
Description | string | Indicates whether or not the Statistics property of StatisticsService.GetStatisticsCollection method will include the time at time when statistics for this BlockStatisticsManifest were first captured.
ModelCorrespondence | string | CIM_BlockStorageStatisticalData.StartStatisticTime
IncludeStatisticTime | boolean | false
Description | string | Indicates whether or not the Statistics property of StatisticsService.GetStatisticsCollection method will include the time when statistics for this BlockStatisticsManifest were last captured.
ModelCorrespondence | string | CIM_BlockStorageStatisticalData.StatisticTime
IncludeTotalIOs | boolean | false
Description | string | Whether to include in a filter for a metered element the cumulative count of I/Os for that element.
ModelCorrespondence | string | CIM_BlockStorageStatisticalData.StatisticTime
IncludeWriteHitIOs | boolean | false
Description | string | Whether to include in a filter for a metered element the cumulative count of Write Cache Hits (Writes that went directly to Cache) for that element.
ModelCorrespondence | string | CIM_BlockStorageStatisticalData.WriteHitIOs
IncludeWriteHitIOTimeCounter | boolean | false
Description | string | Whether to include in a filter for a metered element the cumulative elapsed time for all Write I/Os written to cache for that element.
ModelCorrespondence | string | CIM_BlockStorageStatisticalData.WriteHitIOTimeCounter
IncludeWriteIOs | boolean | false
Description | string | Whether to include in a filter for a metered element the cumulative count of all writes for tat element.
ModelCorrespondence | string | CIM_BlockStorageStatisticalData.WriteIOs
IncludeWriteIOTimeCounter | boolean | false
Description | string | Whether to include in a filter for a metered element the cumulative elapsed time for all Write I/Os for that element.
ModelCorrespondence | string | CIM_BlockStorageStatisticalData.WriteIOTimeCounter
InstanceID | string |
Description | string | Within the scope of the instantiating Namespace, InstanceID opaquely and uniquely identifies an instance of this class. To ensure uniqueness within the NameSpace, the value of InstanceID should be constructed using the following "preferred" algorithm: <OrgID>:<LocalID> Where <OrgID> and <LocalID> are separated by a colon (:), and where <OrgID> must include a copyrighted, trademarked, or otherwise unique name that is owned by the business entity that is creating or defining the InstanceID or that is a registered ID assigned to the business entity by a recognized global authority. (This requirement is similar to the <Schema Name>_<Class Name> structure of Schema class names.) In addition, to ensure uniqueness, <OrgID> must not contain a colon (:). When using this algorithm, the first colon to appear in InstanceID must appear between <OrgID> and <LocalID>. <LocalID> is chosen by the business entity and should not be reused to identify different underlying (real-world) elements. If the above "preferred" algorithm is not used, the defining entity must assure that the resulting InstanceID is not reused across any InstanceIDs produced by this or other providers for the NameSpace of this instance. For DMTF-defined instances, the "preferred" algorithm must be used with the <OrgID> set to CIM.
Key | boolean | true
Override | string | InstanceID
CSVSequence | string[] |
Description | string | The sequence of BlockStorageStatisticalData property names for properties that will be returned are encoded in the CSVSequence array. Properties that are not included will not be returned with GetStatisticsCollection. Properties that are included in CSVSequence will be returned in the order they appear in CSVSequence.
Experimental | boolean | true

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
Description | string | CIM_ManagedElement
ElementName | string | CIM_ManagedElement
Generation | uint64 | CIM_ManagedElement

## Class Methods